; Copyright (C), Intel Corporation. All rights reserved. 
; ********************************************************************************************** 
; **    Filename:  iaStorAC.inf 
; **    Revision:  07/31/2019,15.9.8.1050
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Driver 
; **               Installs: RST AHCI RAID Controller Miniport + RST Filter Driver
; ********************************************************************************************** 
[Version] 
Signature="$Windows NT$" 
Provider=%INTEL% 
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
CatalogFile=iaStorAC.cat
DriverVer=07/31/2019,15.9.8.1050
;
[PackageInfo]
Name=RAID32
;
[SourceDisksNames] 
1 = %DiskId1%,,,"" 
;
[DestinationDirs] 
DefaultDestDir = 12
;
[ControlFlags] 
ExcludeFromSelect = * 
;
[Manufacturer] 
%INTEL% = INTEL, NTx86.6.1, NTx86.6.3, NTx86.10.0
;
[iaStorAC_Service_Inst] 
DisplayName    = %iaStorAC.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER% 
StartType      = %SERVICE_BOOT_START% 
ErrorControl   = %SERVICE_ERROR_NORMAL% 
ServiceBinary  = %12%\iaStorAC.sys 
LoadOrderGroup = SCSI miniport 
AddReg = pnpsafe_pci_addreg
;
[iaStorAC_EventLog_Inst] 
AddReg = iaStorAC_EventLog_AddReg 
;
[iaStorAC_EventLog_AddReg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorAC.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7 
;
[iaStorF_Service_Inst] 
ServiceType = %SERVICE_KERNEL_DRIVER% 
StartType  = %SERVICE_BOOT_START% 
ErrorControl   = %SERVICE_ERROR_NORMAL% 
ServiceBinary  = %12%\iaStorF.sys 
;
[iaStorF_EventLog_Inst] 
AddReg = iaStorF_EventLog_AddReg 
;
[iaStorF_EventLog_AddReg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7 
;
[iaStorF_addreg] 
; Layer the RST Filter driver under all Disk class devices as a lower disk class filter 
;
HKLM, System\CurrentControlSet\Control\Class\{4d36e967-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF 
HKLM, System\CurrentControlSet\Control\Class\{4d36e965-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF 
;
;

;
;******************************************************************************
;*
;* 32-BIT X86 ARCHITECTURE
;*
;* This section specifies the 32-bit architecture specific INF file entries
;* required to install a driver as a 32-bit compatible driver.
;*
;******************************************************************************
[SourceDisksFiles.x86]
iaStorAC.sys = 1,,,
iaStorF.sys = 1,,,

;
;Win7
[INTEL.NTx86.6.1]
%PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_2822&CC_0104
%PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_282A&CC_0104
%PCI\VEN_8086&DEV_9D07&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_9D07&CC_0104
%PCI\VEN_8086&DEV_A107&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_A107&CC_0104
%PCI\VEN_8086&DEV_A106&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_A106&CC_0104
%PCI\VEN_8086&DEV_A28E&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_A28E&CC_0104
%PCI\VEN_8086&DEV_A286&CC_0104.DeviceDesc% = iaStorAC_inst, PCI\VEN_8086&DEV_A286&CC_0104
;
;Win8 and above
[INTEL.NTx86.6.3]
%PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_2822&CC_0104
%PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_282A&CC_0104
%PCI\VEN_8086&DEV_9D07&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_9D07&CC_0104
%PCI\VEN_8086&DEV_A107&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A107&CC_0104
%PCI\VEN_8086&DEV_A106&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A106&CC_0104
%PCI\VEN_8086&DEV_A28E&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A28E&CC_0104
%PCI\VEN_8086&DEV_A286&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A286&CC_0104
;
;Win8 and above
[INTEL.NTx86.10.0]
%PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_2822&CC_0104
%PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_282A&CC_0104
%PCI\VEN_8086&DEV_9D07&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_9D07&CC_0104
%PCI\VEN_8086&DEV_A107&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A107&CC_0104
%PCI\VEN_8086&DEV_A106&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A106&CC_0104
%PCI\VEN_8086&DEV_A28E&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A28E&CC_0104
%PCI\VEN_8086&DEV_A286&CC_0104.DeviceDesc% = iaStorAC_inst_8, PCI\VEN_8086&DEV_A286&CC_0104
;
[iaStorAC_inst.ntx86]
CopyFiles=@iaStorAC.sys
CopyFiles=@iaStorF.sys
FeatureScore=0x80
;
[iaStorAC_inst_8.ntx86]
CopyFiles=@iaStorAC.sys
FeatureScore=0x80
;
[iaStorAC_inst.ntx86.HW]
AddReg = iaStorF_addreg
AddReg = msi_addreg
AddReg = storport_addreg
AddReg = etw_rst
;
[iaStorAC_inst_8.ntx86.HW]
AddReg = msi_addreg
AddReg = storport_addreg
AddReg = etw_rst
;
[iaStorAC_inst.ntx86.Services]
AddService = iaStorAC, %SPSVCINST_ASSOCSERVICE%, iaStorAC_Service_Inst, iaStorAC_EventLog_Inst
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst
;
[iaStorAC_inst_8.ntx86.Services]
AddService = iaStorAC, %SPSVCINST_ASSOCSERVICE%, iaStorAC_Service_Inst, iaStorAC_EventLog_Inst
;******************************************************************************
;
;
;
[pnpsafe_pci_addreg]
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars 
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb
HKR, Parameters\PnpInterface,  5,  %REG_TYPE_DWORD%,  0x00000001 
HKR, Parameters, BusType, %REG_TYPE_DWORD%,  0x00000008
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8)
HKR, Parameters\Device, EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001
;
; Opt into StorPort's I/O latency cap.
HKR, "Parameters",             "IoLatencyCap",              %REG_TYPE_DWORD%,  0x000001F4 
;
[Strings] 
; Localizable Strings 
diskId1 = "RST Installation Disk" 
;
; Client devices
iaStorAC.DeviceDesc                      = "Intel(R) Chipset SATA/PCIe  RST Premium Controller"
PCI\VEN_8086&DEV_2822&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_282A&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_9D07&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_A107&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_A106&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_A28E&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
PCI\VEN_8086&DEV_A286&CC_0104.DeviceDesc = "Intel(R) Chipset SATA/PCIe RST Premium Controller"
;
INTEL = "Intel Corporation"
;
; Non-Localizable Strings 
SPSVCINST_ASSOCSERVICE = 0x00000002 
REG_TYPE_SZ = 0x00000000 
REG_MULTI_SZ = 0x00010000 
REG_EXPAND_SZ = 0x00020000 
REG_TYPE_DWORD = 0x00010001 
SERVICE_KERNEL_DRIVER  = 1 
SERVICE_FILE_SYSTEM_DRIVER = 2
SERVICE_WIN32_OWN_PROCESS = 0x00000010
SERVICE_BOOT_START = 0
SERVICE_AUTO_START = 2
SERVICE_DEMAND_START = 3
SERVICE_ERROR_NORMAL   = 1
;

;
; MSI enables. 
[msi_addreg]
HKR, Interrupt Management, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported, %REG_TYPE_DWORD%,   1
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   80
HKR, Interrupt Management\Affinity Policy, 0x00000010
HKR, Interrupt Management\Affinity Policy, DevicePolicy, %REG_TYPE_DWORD%, 5 ;IrqPolicySpreadMessagesAcrossAllProcessors
;
[storport_addreg]
; Enables/Disables Idle Power Management for StorPort
HKR, StorPort, EnableIdlePowerManagement, %REG_TYPE_DWORD%, 0x00000001
; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255)
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF
;
[etw_rst]
; Configuring and Starting an AutoLogger Session
;   LogFileMode = Buffering Mode
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, LogFileMode, %REG_TYPE_DWORD%, 0x00000400
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, FileName
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, Guid, %REG_TYPE_SZ%, "{347659f2-c334-46ab-b19e-a451e851c695}"
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, Start, %REG_TYPE_DWORD%, 0x00000001
; Configure provider using GUID
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableProperty, %REG_TYPE_DWORD%, 0x00000000
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, Enabled, %REG_TYPE_DWORD%, 0x00000001
;   Level = TRACE_LEVEL_INFORMATION
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableLevel, %REG_TYPE_DWORD%, 0x00000004
;   Flags = ALL
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableFlags, %REG_TYPE_DWORD%, 0x0000FFFF