; SoundMAX device information file for ODM
; Analog Devices, Inc. Copyright(c) 1998 - 2007
; SoundMAX package [1V]

[Version]
Signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
provider=%ANLG%
DriverVer = 05/29/2007,%DriverBuildID%
CatalogFile=smx.cat

; nat27 prepared for NT6x64_PE 06-May-2013

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MfgName%=AnalogDevices, NTamd64

[AnalogDevices.NTamd64]

%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1039&dev_7012&subsys_81391043
;
; CH4 DriverVer = 10/12/2006,DriverBuildID="5.12.01.5410"
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02011179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02021179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02031179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02041179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02051179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00011179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_FF101179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02411179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02421179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02431179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02441179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02461179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_FFFF1179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02491179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_FF201179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02C51179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02C61179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02451179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02511179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02521179
; CH6 DriverVer = 10/12/2006,DriverBuildID="5.12.01.5410"
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02471179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02411179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02481179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_FF001179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_FF101179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02531179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02541179
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02C61179
;
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2485&subsys_04201558
; FSC
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_266E&subsys_105A1734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_1106&dev_3059&subsys_0079110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_1106&dev_3059&subsys_11C210CF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2425&subsys_0048110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_7195&subsys_0048110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2425&subsys_0049110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_7195&subsys_0049110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2425&subsys_004011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_7195&subsys_004011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2415&subsys_004811D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_2425&subsys_004811D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_7195&subsys_004811D4
; ASUS - VIA\INTEL
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_8086&dev_24D5&subsys_80B01043 ;p4p800-F
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1106&dev_3059&subsys_80A11043 ;a7v880
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1106&dev_3059&subsys_80B01043 ;a7v880
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1106&dev_3059&subsys_59301462 ;a7v880
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1106&dev_3059&subsys_810D1043 ;a7v880
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_8086&dev_24D5&subsys_42368086 ;p4pex
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_8086&dev_24D5&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_82271043 ;P5PEVM
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_8086&dev_24D5&subsys_90541509
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_8086&dev_24D5&subsys_92011509
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_1106&dev_3059&subsys_537011D4 ;a7v880
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_8086&dev_24D5&subsys_75801462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_00951071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_11471071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_10951071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_20951071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_218114A4
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_8086&dev_24D5&subsys_81011043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_01121071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_218814A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_53754144 ;p4p800se
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_A0001458 ;p4p800se
%*WDM_AC97AUD.DeviceDesc%=WDM_ASUS,     pci\ven_8086&dev_24D5&subsys_80F31043 ;p4p800se
%*WDM_AC97AUD.DeviceDesc%=WDM_ASUS,     pci\ven_8086&dev_24D5&subsys_81521043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_01471071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_21471071
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_8086&dev_24D5&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_8086&dev_24D5&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_8086&dev_24D5&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_8086&dev_24D5&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_D1101071
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_A6001458
%*WDM_AC97AUD.DeviceDesc%=WDM_M188,     pci\ven_8086&dev_24D5&subsys_71281462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_11280923
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE,      pci\ven_8086&dev_24D5&subsys_003715D4
%*WDM_AC97AUD.DeviceDesc%=WDM_A1986A,   pci\ven_8086&dev_24D5&subsys_818F1043
; INTEL - SYS
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1039&dev_7012&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_A188,     pci\ven_1039&dev_7012&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMSPDFN, pci\ven_1039&dev_7012&subsys_537011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_ODMNOSPF, pci\ven_1039&dev_7012&subsys_806A1043
%*WDM_AC97AUD.DeviceDesc%=WDM_ASUS,     pci\ven_1039&dev_7012&subsys_80F31043
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3,      pci\ven_1039&dev_7012&subsys_1B271019
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_1039&dev_7012&subsys_01883411
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_1039&dev_7012&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_1039&dev_7012&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_SF3LEN,   pci\ven_1039&dev_7012&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_VM5,      pci\ven_1039&dev_7012&subsys_01951028
%*WDM_AC97AUD.DeviceDesc%=WDM_M188,     pci\ven_1039&dev_7012&subsys_71281462
%*WDM_AC97AUD.DeviceDesc%=WDM_M188,     pci\ven_1039&dev_7012&subsys_D61F8086 ;D201GLY2(A)
%*WDM_AC97AUD.DeviceDesc%=WDM_A1986A,   pci\ven_1039&dev_7012&subsys_818F1043
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_18801019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_18791019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_18781019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_18771019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_1B961019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_21041019
%*WDM_AC97AUD.DeviceDesc%=WDM_M939,     pci\ven_1039&dev_7012&subsys_21051019
%*WDM_AC97AUD.DeviceDesc%=WDM_CPAL188,  pci\ven_1039&dev_7012&subsys_00911025
%*WDM_AC97AUD.DeviceDesc%=WDM_T19,      pci\ven_1039&dev_7012&subsys_11931043
%*WDM_AC97AUD.DeviceDesc%=WDM_M1981B,   pci\ven_1039&dev_7012&subsys_71971462
%*WDM_AC97AUD.DeviceDesc%=WDM_T19,      pci\ven_1039&dev_7012&subsys_C0131631
%*WDM_AC97AUD.DeviceDesc%=WDM_HRR,      pci\ven_1039&dev_7012&subsys_82101033
%*WDM_AC97AUD.DeviceDesc%=WDM_K1,       pci\ven_1039&dev_7012&subsys_820F1033
;
; Sound B 10.09 [Bashrat the Sneaky]
;
; S10\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01D51028
;
; Sound B 10.03 [Bashrat the Sneaky] 
;
; S53\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_02671014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_027E1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_026A1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_027A1014
;
; S41\smwdmVI3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_90521509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_90071509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_22013411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_80F31043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_202B161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_88011849
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_A2001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_A2001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_A6001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_A6001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_86663411
;
; Sound B 8.05 [Bashrat the Sneaky] 
;
; SMA8\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_90431509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_90441509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_902A1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_902B1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_12101462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_55511462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A2001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A2001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A6001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A6001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_71281462
;
; SMA8\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_811F1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_80F31043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3081103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_309E103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_309D103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_03601462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_303017AA
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_0938103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_71281462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_204A161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_204C161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_00201170
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_500617FF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_FFE01170
;
; SMAH\smwdm.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_104311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_104311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_11D41043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_104311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_104311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_11D41043
;
; SMF\smwdmCH1.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_004011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_0048110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_0056110A
;
; SMF\smwdmCH2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_004011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0048110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0049110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0088110A
;
; SMF\smwdmVI6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_118710CF
;
; SMF2\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00881734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_10231734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_118910CF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_11E410CF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_121810CF
;
; SMF2\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_10221734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_10211734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_10201734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_122F10CF
;
; SMF3\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_10281734
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_10291734
;
; IB\smwdmCH3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_05081014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_051C1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_051F1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_05001014
;
; IB2\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05231014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05371014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05541014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_055F1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05341014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05421014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05731014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_05581014
;
; IB2\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_05671014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_057F1014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_05801014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_05811014
;
; IB4\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_02871014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_02851014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_02C71014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_02D21014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_02B31014
;
; IB4\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02B51014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02B61014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02D81014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02D91014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02D11014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02F81014
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_02F71014
;
; SMA1\smwdmHRP.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_25A6&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_25A6&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_25A6&subsys_80F31043
;
; SMA2\smwdmATI.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_E00D1631
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_18331043
;
; SMA4\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_537011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_81011043
;
; SMA6\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_41445375
;
; SMA7\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_0940103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_0934103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_0944103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_099C103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3088103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_300F103C
;
; SMA8\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_90431509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_90441509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_902A1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_902B1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_12101462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_55511462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A2001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A2001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A6001940
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_A6001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_71281462
;
; SMA8\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_810D1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_811F1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_80F31043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3081103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_309E103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_309D103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_03601462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86663411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86661019
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86668086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_86661462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_303017AA
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_0938103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_71281462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_204A161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_204C161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_00201170
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_500617FF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_FFE01170
;
; SMAB\smwdmAL3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5455&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5455&subsys_810D1043
;
; SMAE\smwdmAT4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_00301170
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_71281462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_2043161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_2044161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_2041161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_201917C0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_11831043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_00911025
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4370&subsys_001214C0
;
; SMAJ\smwdmATI.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_B02A144D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1002&dev_4341&subsys_B028144D
;
; SMC1\smwdm.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1810E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1820E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1830E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1840E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1850E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1860E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1870E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1880E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1890E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1970E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1980E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1A50E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1A60E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1B40E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1BF0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B1730E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_B19F0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_05C00E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_05F40E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_065C0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_002F0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00300E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00310E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_B1940E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_003D0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_00AB0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00720E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_00340E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_008E0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_008F0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_00920E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_00960E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00970E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00A00E11
;
; SMC2\smwdmALI.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_00B00E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_00560E11
;
; SMC2\smwdmCH3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_005C0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_004A0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_004E0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_00B70E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_00570E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_00B40E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_007B0E11
;
; SMD2\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_03011028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_03031028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01261028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01271028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_012C1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_012D1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01291028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_013A1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01461028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01481028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01421028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01601028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01611028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01331028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01321028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01381028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_015E1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_013D1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_014B1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01471028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01981028
;
; SMD2\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01511028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01691028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01681028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_03021028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01541028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01551028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01571028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01741028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01761028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01561028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01621028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_017A1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_019D1028
;
; SMD2\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01771028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01811028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01991028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_017B1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01781028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01791028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01751028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01901028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_01A11028
;
; SMD2\smwdmCH7.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_27DE&subsys_01AD1028
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_27DE&subsys_01BC1028
;
; SMD3\smwdmSIS.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1039&dev_7012&subsys_88011849
;
; SME\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_4000107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2000107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_500E107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_5288107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2009107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2011107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_1049107B
;
; SMG\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_2018107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_2019107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_2026107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_2023107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_0865107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_0875107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_1865107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_1875107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_7147107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_7148107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_4042107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_2024107B
;
; SMG3\smwdm.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_0008107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_3400107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_3400107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3400107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_9047107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_0106107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0111107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3600107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_500D107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_1020107B
;
; SMG7\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_182C1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_18031043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_18231043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2030161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_202D161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_D80417AA
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_18731043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_500417FF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_500517FF
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_000A1170
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_000B1170
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2035161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_3089103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_2039161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_203A161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_203B161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_203E161F
;
; SMH2\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3005103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3006103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3007103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_3008103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_300A103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_300B103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_300C103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_300D103C
;
; SMH3\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00580E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_088C103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_08A8103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_0890103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_08BC103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_08600E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_08B0103C
;
; SMH4\smwdmCH2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00070E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00080E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00090E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000B0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000C0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000D0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000E0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000F0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00100E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00880E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00890E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_008B0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_008C0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_008D0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00A50E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00A60E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00A70E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_000A0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_008A0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_124C103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_80101043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_890D1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_1274103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_126E103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_126F103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_1279103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_127A103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_806A1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3084109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3181109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_80761043
;
; SMH4\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00BA0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00B80E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00C40E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00AD0E11
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_00C3103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_1296103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_1298103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_808E1043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_12F0103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_3187109F
;
; SMH4\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_12BC103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_12BF103C
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_12BD103C
;
; SMH4\smwdmNV2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10DE&dev_006A&subsys_12B9103C
;
; SMH4\smwdmNV8.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10DE&dev_00DA&subsys_12BB103C
;
; SMH5\smwdmCH6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_266E&subsys_203D161F
;
; SMIN\smwdmCH0.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_42578086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_59418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_43418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_46428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_1401107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_42418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_41538086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_47538086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_42508086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_9019107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_1400107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_4F528086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_53558086
;
; SMIN\smwdmCH1.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_59418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_42418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_4F528086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_43418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_41538086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_42578086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_47538086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_42508086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_53558086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_46428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_45418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_9019107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_1400107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_1401107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_47428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_424E8086
;
; SMIN\smwdmCH2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_45418086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_47428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_424E8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_43338086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_484D8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_54428086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_50548086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_70748086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_57528086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_45328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_46568086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_45578086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_47328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_4D568086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_4D448086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_6D768086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_6D648086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_4D328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_324D8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_6D328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_48568086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_574E8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_68768086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_776E8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_42478086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_62678086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_010A8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_010B8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_010C8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_010D8086
;
; SMIN\smwdmCH3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_19698086
;
; SMIN\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_46548086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_46488086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01038086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01048086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01058086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01068086 ;INTEL D845PESV
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01078086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01088086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_010A8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_010B8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_010C8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_010D8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_50328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42328086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_536011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42548086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42368086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01098086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_42478086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_537111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_537211D4
;
; SMIN\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_20008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_20018086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_20028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_40008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_40018086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_40028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60018086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60038086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60048086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60058086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60068086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60078086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60088086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_60098086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_A0008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_A0018086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_A0028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0018086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0038086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0048086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0058086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0078086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0088086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0098086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00C8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00D8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00E8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00F8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0108086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0118086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0128086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0028086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0068086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00A8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00B8086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E8008086
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E8018086
;
; SMIN\smwdmHRP.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_25A6&subsys_53744144
;
; SMM\smwdmCH5.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E0081631
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_76301462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01611462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_E00A1631
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24D5&subsys_01601462
;
; SMS\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_8144104D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_8172104D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_8198104D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_8197104D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_81C0104D
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_81C5104D
;
; SMZ\smwdmALI.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_202A161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_2027161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_2028161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_10B9&dev_5451&subsys_2029161F
;
; SMZ\smwdmCH0.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_536111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2425&subsys_534011D4
;
; SMZ\smwdmCH1.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_536111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_7148109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_3187109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_534011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_536011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_154811D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_99161509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_38151DE1
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_11D41043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_0049110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_211814A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_000F1025
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_63701462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_215414A4
;
; SMZ\smwdmCH2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_536111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3180109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3182109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3183109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_7145109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_7146109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_901D1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_3184109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_300E14CD
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_714A109F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_90291509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_214714A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_212614A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_001415D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_534011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_536011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_456011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0040A0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_00EEA0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_11D41043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_24451054
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_35101462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0056110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_112110Cf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_89131509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_30051695
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_81301033
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_214914A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_890C1509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0086A0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0122107B
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_21C414CD
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_300314CD
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_300414CD
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_33911462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_52301462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_215014A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_4D263411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_52213411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_52223411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_52243411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_53193411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_56193411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_561A3411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_561E3411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_56203411
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0152A0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_20321025
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_215614A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_0004109F
;
; SMZ\smwdmCH3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_536111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_04601558
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_18411509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_0089110A
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_534011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_536011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_075715D5
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2485&subsys_537411D4
;
; SMZ\smwdmCH4.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_0237A0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_01FAA0A0
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_002815D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_217914A4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_24C5&subsys_57101462
;
; SMZ\smwdmMX0.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_7195&subsys_534011D4
;
; SMZ\smwdmVI3.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_03203116
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3059&subsys_59301054
;
; SMZ\smwdmVI6.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_536111D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_536311D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_A0001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_201A161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_18401509
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_2025161F
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_534011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_586011D4
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_00291025
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_58301054
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_30581054
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_36821462
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_1106&dev_3058&subsys_536011D4
;
; SMZ2\smwdmCH2.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_A0001458
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_80B01043
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2445&subsys_537011D4
;
; SMZ4\smwdm.inf
%*WDM_AC97AUD.DeviceDesc%=WDM_XPE, pci\ven_8086&dev_2415&subsys_01141028

[DestinationDirs]
DefaultDestDir = 10,system32\drivers   ; %SystemRoot%\system32\drivers
WDM_AC97AUD.CopyList = 10,system32\drivers   ; %SystemRoot%\system32\drivers

[WDM_AC97AUD.DelReg]
HKR, Drivers
HKR, Disable
HKR, Settings
HKR, Sensaura\Configuration

[WDM_AC97AUD.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,smwdm.sys
HKR,,NTMPDriver,,"smwdm.sys,sbemul.sys"

HKR,Drivers,SubClasses,,"wave,midi,mixer"

HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv, Description,,%*WDM_AC97AUD.DeviceDesc%
HKR,Drivers\midi\wdmaud.drv, Description,,%WDM_MIDI%
HKR,Drivers\mixer\wdmaud.drv,Description,,%*WDM_AC97AUD.DeviceDesc%

; Establish max/min values for Volume nodes. "xxxxMax" is the setting for
;  maximum volume level (minimum attenuation). "xxxxMin" is the setting for
;  minimum volume level (maximum attenuation). These values are the Max/Min
;  bits written to the register for the Max/Min level. As an example, the
;  MicIn maximum volume can be set to 2 which equals a maximum output of +9 db,
;  the MicIn minimum is set to 10 which equals a minimum output of - 12 db.
;  (All register values are Hex.)

HKR, Settings, "SurVMax", 1, 08   ;   Surround Volume
HKR, Settings, "CtrVMax", 1, 08   ;   Center Volume
HKR, Settings, "LfeVMax", 1, 08   ;   Lfe Volume ( sub woofer )

; Max/Min record levels. xxxRMax is the maximum gain code for that record
;  source. xxxRMin is the minimum gain code for that source.

; Default volume / mute settings. These are the initial installation settings.
; The volume default values are tested againts the Max/Min values that may have
;  been previously established. The Boolean settings (Mute, 20 db, etc.) are
;  set as 0 = FALSE, non-zero = TRUE;
;
; Note that a particular hardware platform may not implement all signal paths.
;
; This is the mixed digital PCM stream (Wave, SW Synth and Digital Redbook)
; This setting is not adjustable from a Mixer control slider. This is
; not adjustable from the Mixer applet.
HKR, Settings, "NULL", 1, 00     ;   Generic handler for un-named nodes

HKR, Settings, "MasM", 1, 00     ;   Master Mute
HKR, Settings, "MasV", 1, 08     ;   Master Volume
HKR, Settings, "PCBV", 1, 08     ;   PCBeep Volume
HKR, Settings, "PCBM", 1, 00     ;   PCBeep Mute
                                    
HKR, Settings, "PhoV", 1, 08     ;   Phone Volume
HKR, Settings, "VidV", 1, 08     ;   Video Volume
HKR, Settings, "AuxV", 1, 08     ;   Aux Volume

HKR, Settings, "MicM", 1, 01     ;   Mic In Mute
HKR, Settings, "MicS", 1, 00     ;   Mic In Select (0 == Mic1, 1 == Mic2)

HKR, Settings, "P3DV", 1, 0A     ;   Stereo Wide (Phat 3D) Volume ( 0 - F )
HKR, Settings, "P3DB", 1, 01     ;   Use enhancement on digital streams
HKR, Settings, "MonV", 1, 08     ;   Mono Out Volume
HKR, Settings, "RecS", 1, 00     ;   Record source (0=Mic, 1=CD, 2=Vid, 3=Aux
                                 ;      4=LineIn, 5=WaveOut, 6=MonoOut, 7=Phone

HKR, Settings, "FntV", 1, 08     ;   Surround Volume
HKR, Settings, "SurV", 1, 08     ;   Surround Volume
HKR, Settings, "LfeV", 1, 08     ;   Lfe Volume ( sub woofer )

HKR, Settings, "AltMicSelect", 1, 01  ; Define MS as an On/Off control
HKCU,Software\Microsoft\Multimedia\Audio,DefaultFormat,,"Default Quality"
HKCU,Software\Microsoft\Multimedia\Audio\WaveFormats,"Default Quality",1, 01,00,02,00,44,AC,00,00,10,B1,02,00,04,00,10,00

; Record Controls

HKR, Settings, "ACDR", 1, 01     ;   CD (Analog CD, not Redbook Audio)
HKR, Settings, "VidR", 1, 01     ;   Video
HKR, Settings, "AuxR", 1, 01     ;   Aux
HKR, Settings, "LinR", 1, 01     ;   Line In
HKR, Settings, "MonR", 1, 01     ;   Mono output loopback
HKR, Settings, "PhoR", 1, 01     ;   Phone
; Enable Interrupt on each processed BDL
;  00 = Interrupt only when KMixer request
;  01 = Interrupt on every BDL
HKR, Settings, "SGUpdate", 1, 01

; Disable Node display on mixer applet. Set to 00 to enable, 01 to disable.
HKR, Disable, "NULL", 1, 00     ;   Generic handler for un-named nodes
HKR, Disable, "20db", 1, 00     ;   Mic 20db Gain
HKR, Disable, "MicV", 1, 00     ;   Mic In Volume
HKR, Disable, "MicM", 1, 00     ;   Mic In Mute

; Record Controls
HKR, Disable, "MicR", 1, 00     ;   Mic
HKR, Disable, "OutR", 1, 00     ;   Line output loopback
;If you want the MonoOut to track the Master Volume control, set MonoWithMaster
;to 01. If you want separate Master Volume and MonoOut controls, set
;MonoWithMaster to 00. If MonoWithMaster = 01, the "MonoOut" controls will _not_
;be present on SndVol32 (the Master Volume control will control the MonoOut
;output)

;If a AD1885/6 is detected and you want the (headphone) amplifier to track the
;Master Volume control, set HPWithMaster to 01 (same code written to Master
;Volume and Headphone volume based upon Master volume settings). If you want
;separate controls for the Master Volume and Headphone, set HPWithMaster to 00.
;If ;HpWithMaster = 01, the "Headphone" controls will _not_ be present on
;SndVol32 (the Master Volume control will control the Headphone amplifier output)
;If HpWithMaster = 01, the following INF settings are ignored, HP_VMax, HP_VMin,
;HP_V, HP_M, HP_P.
;An AD1887 uses the settings for the Master Volume to control the output and
;automatically sets HPWithMaster.

;If a AD1885/6 is detected and the (headphone) amplifier is used, set HP_P to 00.
;If the amplified output is not used, set HP_P to 01. If you selected
;HPWithMaster, this setting is interpreted to be 01 (not active).

[SPDIFOff.AddReg]
HKR, Disable, "SPDF", 1, 01     ;   01 = Disabled (default), 00 = Enabled

[SPDIFLAP.AddReg]
; Enable/Disable the S\PDIF channel
HKR, Disable, "SPDF", 1, 00     ;   01 = Disabled (default), 00 = Enabled
; S/PDIF channel Data Type
HKR, Settings, "CAC3",  1, 01   ;   00 = AC3 not checked (default), 01 = AC3 checked
HKR, Settings, "CPCM",  1, 01   ;   00 = PCM not checked (default), 01 = PCM checked

[ODMFVMax.AddReg]
HKR, Settings, "FntVMax",            1, 08   ;   Front Volume
HKR, Settings, "PCMOutVolume",       1, 08 ; PCM Out volume 8 = 0db gain, 7 = +1.5db

[ODMFVM2.AddReg]
HKR, Settings, "FntVMax",            1, 07   ;   Front Volume
HKR, Settings, "PCMOutVolume",       1, 07 ; PCM Out volume 8 = 0db gain, 7 = +1.5db

[LinVCom.AddReg]
HKR, Settings, "LinV", 1, 08     ;   LineIn Volume

[OdmCom.AddReg]
HKR, Settings, "CtrV",              1, 08 ; Center Volume

[Odm.AddReg]
;Apply for AD198x codecs.  Ability to swap control and data.
HKR, Disable, "SWPC",               1, 00 ; control enabled
HKR, Disable, "SWPD",               1, 00 ; control enabled

HKR, Settings, "SwapCenterLFE",     1, 02 ; Swap the data when the control is swapped

[OdA18.AddReg]
HKR, Disable, "SWPC",               1, 00 ; control enabled
HKR, Disable, "SWPD",               1, 00 ; control enabled

HKR, Settings, "SwapCenterLFE",     1, 03 ; Swap the data when the control is swapped
HKR, Settings, "SWPC",              1, 01 ; Controls not swapped

[AusCom.AddReg]
HKR, Settings, "ACDRMax",           1, 0A ; Max Analog CD Gain (not Redbook Audio)
HKR, Settings, "AuxRMax",           1, 0A ; Aux
HKR, Settings, "CtrV",              1, 00 ; Center Volume
HKR, Settings, "LinRMax",           1, 0A ; Line In

[A188M.AddReg]
HKR, Settings, "SPDIFBit",          1, 00 ; Always set the Copy Protection Bit to 0

[M533.AddReg]
HKR, Settings, "JackSenseConf",     1, C1, 20, F6, FF
HKR, Settings, "JackSenseShare",    1, FF, 57, FF, FF

[A188.AddReg]
HKR, Settings, "JackSenseConf",     1, C1, 20, F6, FF
HKR, Settings, "JackSenseShare",    1, FF, 75, FF, FF
HKR, Settings, "SPDIFBit",          1, 00 ; Always set the Copy Protection Bit to 0

[Sf3Len.AddReg]
HKR, Disable, "SWPC",            1, 00 ; control enabled
HKR, Disable, "SWPD",            1, 00 ; control enabled

HKR, Settings, "JackSenseConf",  1, C1, 20, F6, FF
HKR, Settings, "JackSenseShare", 1, FF, 57, FF, FF
HKR, Settings, "MagicNumber",    1, 00, 30, 00, 40
HKR, Settings, "SPDIFBit",       1, 00 ; Always set the Copy Protection Bit to 0
HKR, Settings, "SwapCenterLFE",  1, 02 ; Swap the data when the control is swapped
HKR, Settings, "SWPC",           1, 01 ; Controls swapped

[Js_JeA.AddReg]
HKR, Settings, "ACDRMAX",     1, 0A ; CD (Analog CD, not Redbook Audio)
HKR, Settings, "AuxRMAX",     1, 0A ; Aux
HKR, Settings, "CtrV",        1, 00 ; Center Volume
HKR, Settings, "LinRMAX",     1, 0A ; Line In
HKR, Settings, "LockMSToOMS", 1, 01 ; Causes left/right swap of stereo microphone input when OMS bit is set.
HKR, Settings, "SPDIFBit",    1, 00 ; Always set the Copy Protection Bit to 0
HKR, Settings, "StereoMic",   1, 01 ; 00 = mono mic support, 01 = stereo mic support
HKR, Settings, "SWPC",        1, 01 ; Controls not swapped

[P4Com.AddReg]
HKR, Disable, "AuxM",               1, 01 ; Aux Mute
HKR, Disable, "AuxR",               1, 01 ; Aux Record
HKR, Disable, "AuxV",               1, 01 ; Aux Volume
HKR, Settings, "AuxM",              1, 01 ; Aux Mute

[M188.AddReg]
HKR, Disable, "AuxM", 1, 01 ; Aux Mute
HKR, Disable, "AuxR", 1, 01 ; Aux Record
HKR, Disable, "AuxV", 1, 01 ; Aux Volume
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "PhoM", 1, 01 ; Phone Mute
HKR, Disable, "PhoR", 1, 01 ; Phone Volume
HKR, Disable, "PhoV", 1, 01 ; Phone Volume

HKR, Settings, "AuxM", 1, 01 ; Aux Mute
HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "PhoM", 1, 01 ; Phone Mute 

[OdmSiS.AddReg]
HKR, Settings, "3dBBoost",          1, 01, 00, 00, 00
HKR, Settings, "HPWithMaster",      1, 01 ; 00 = Normal, 01 = Amplifier output tracks Master
HKR, Settings, "MagicNumber",       1, 00, 30, 00, 40
HKR, Settings, "MicR",              1, 08 ; Mic
HKR, Settings, "MuteSplitEnab",     1, 00 ; Mute split (0= disable, 1=enable)
HKR, Settings, "VRefLevel",         1, 01 ; AD1981A VRefLevel. 00 = 2.25v, 01 = 3.7v

[AusSiS.AddReg]
HKR, Settings, "3dBBoost",          1, 01, 00, 00, 00
HKR, Settings, "CalPin",            1, 1F ; Disables calibration
HKR, Settings, "HPWithMaster",      1, 01 ; 00 = Normal, 01 = Amplifier output tracks Master
HKR, Settings, "MagicNumber",       1, 00, 30, 00, 60
HKR, Settings, "MicR",              1, 08 ;  Mic
HKR, Settings, "MuteSplitEnab",     1, 00 ; Mute split (0= disable, 1=enable)

[Odm8S.AddReg]
HKR, Settings, "MagicNumber",       1, 00, 30, 00, 40

[VM5.AddReg]
HKR, Disable, "ACDV", 1, 01 ; Analog CD Volume (not digital redbook !)
HKR, Disable, "ACDM", 1, 01 ; Analog CD Mute
HKR, Disable, "ACDR", 1, 01 ; CD (Analog CD, not Redbook Audio)
HKR, Disable, "LinV", 1, 01 ; LineIn Volume
HKR, Disable, "LinM", 1, 01 ; LineIn Mute
HKR, Disable, "LinR", 1, 01 ; Line In
HKR, Disable, "MicS", 1, 01 ; Mic In Select
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume

HKR, Settings, "ACDM", 1, 01 ; Analog CD Mute
HKR, Settings, "LinM", 1, 01 ; LineIn Mute
HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "StereoMic", 1, 01 ; 00 = mono mic support, 01 = stereo mic support

[Js_Je.AddReg]
; Jack Sharing + Jack Enumeration
HKR, Disable,  "MicS",             1, 00 ; Mic In Select
HKR, Settings, "JackSenseConf",	   1, C1, 20, F6, FF
HKR, Settings, "JackSenseInhibit", 1, F1, FF, FF, FF
HKR, Settings, "JackSenseShare",   1, FF, 57, FF, FF

[Js_Jesis.AddReg]
; Jack Sharing + Jack Enumeration
HKR, Disable,  "MicS",             1, 00 ; Mic In Select
HKR, Settings, "JackSenseShare",   1, FF, 57, FF, FF
HKR, Settings, "JackSenseConf",    1, 11, 20, 5F, FF

[ODMSiS_A.AddReg]
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "PhoM", 1, 01 ; Phone Mute
HKR, Disable, "PhoR", 1, 01 ; Phone Volume
HKR, Disable, "PhoV", 1, 01 ; Phone Volume

HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "PhoM", 1, 01 ; Phone Mute 
HKR, Settings, "JackSenseVref", 1, FF, 4F, 4F, FF
HKR, Settings, "JackSense", 1, 10, 08, 00, 00
HKR, Settings, "JackSense2", 1, 30, 00, 00, 00
HKR, Settings, "LinM", 1, 01 ; Mute Lin In function in playback
HKR, Settings, "ImpedanceReduce",1,01 ; reduce impedance sense and measurement pulse width 

[Js_JeB.AddReg]
HKR, Settings, "JackSense", 1, 50, 00, 00, 00
HKR, Settings, "JackSense2", 1, F0, 02, 00, 00

[Sf3Com.AddReg]
HKR, Settings, "3dBBoost",       1, 01, 00, 00, 00
HKR, Settings, "HPWithMaster",   1, 01 ; 00 = Normal, 01 = Amplifier output tracks Master
HKR, Settings, "VRefLevel",      1, 01 ; AD1981A VRefLevel. 00 = 2.25v, 01 = 3.7v

[Sf3.AddReg]
HKR, Settings, "3Jack",          1, 03 ; 3 Jack sharing. 03 = 2 channel mode
HKR, Settings, "JackSenseConf",  1, F1, 75, FF, FF

[Z94L.AddReg]
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "AuxM", 1, 01 ;
HKR, Disable, "AuxR", 1, 01 ;
HKR, Disable, "AuxV", 1, 01 ;
HKR, Disable, "LinM", 1, 01 ;
HKR, Disable, "LinR", 1, 01 ;
HKR, Disable, "LinV", 1, 01 ;
HKR, Disable, "HP_M", 1, 01 ;
HKR, Disable, "HP_V", 1, 01 ;

HKR, Settings, "HP_M", 1, 01 ;
HKR, Settings, "LinM", 1, 01 ;
HKR, Settings, "AuxM", 1, 01 ;
HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "3Jack", 1, 03 ; Use Stereo Mode
HKR, Settings, "HP_LOSwap", 1, 00; No swap (LO plays front data, HP plays rear data)
HKR, Settings, "20db", 1, 01; Enable Mic 20db Gain by Default.
HKR, Disable,  "MicS", 1, 01 ; Mic In Select
HKR, Settings, "CtrM", 1, 00     ;   Center Mute
HKR, Settings, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )
HKR, Settings, "FntM", 1, 00     ;   Surround Mute
HKR, Settings, "SurM", 1, 00     ;   Surround Mute

[ODMSiS_M.AddReg]
HKR, Settings, "CtrM", 1, 00     ;   Center Mute
HKR, Settings, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )
HKR, Settings, "FntM", 1, 00     ;   Surround Mute
HKR, Settings, "HP_M", 1, 00     ;   Headphone Mute
HKR, Settings, "SurM", 1, 00     ;   Surround Mute

[P4VCom.AddReg]
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "PhoM", 1, 01 ; Phone Mute
HKR, Disable, "PhoR", 1, 01 ; Phone Volume
HKR, Disable, "PhoV", 1, 01 ; Phone Volume

HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "PhoM", 1, 01 ; Phone Mute

[M939.ADDREG]
HKR, Disable, "MicS", 1, 00 ; Mic In Select
HKR, Settings, "AuxM", 1, 01 ; Aux Mute
HKR, Settings, "JackSense", 1, 00, 10, 00, 00
HKR, Settings, "CtrV", 1, 08 ; Center Volume
HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "PhoM", 1, 01 ; Phone Mute

[CPAL188.AddReg]
HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "AuxM", 1, 01 ; 
HKR, Settings, "LinM", 1, 01 ; 
HKR, Settings, "Mics", 1, 00; 0(MIC1), 1(MIC2)
HKR, Settings, "3Jack", 1, 03 ; Use Stereo Mode
HKR, Settings, "20db", 1, 01; Enable Mic 20db Gain by Default.
HKR, Settings, "SPDIFBit",          1, 00 ; Always set the Copy Protection Bit to 0

HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "AuxM", 1, 01 ; 
HKR, Disable, "AuxR", 1, 01 ; 
HKR, Disable, "AuxV", 1, 01 ; 
HKR, Disable, "LinM", 1, 01 ; 
HKR, Disable, "LinR", 1, 01 ; 
HKR, Disable, "LinV", 1, 01 ; 
HKR, Disable, "MicS", 1, 00 ; Mic In Select

[M1981B.AddReg]
HKR, Disable, "MonM", 1, 01 ; Mono Out Mute
HKR, Disable, "MonR", 1, 01 ; Mono output loopback
HKR, Disable, "MonV", 1, 01 ; Mono Out Volume
HKR, Disable, "PhoM", 1, 01 ; Phone Mute
HKR, Disable, "PhoR", 1, 01 ; Phone Volume
HKR, Disable, "PhoV", 1, 01 ; Phone Volume
HKR, Disable, "MicS", 1, 01 ; Mic In Select

HKR, Settings, "MonM", 1, 01 ; Mono Out Mute
HKR, Settings, "PhoM", 1, 01 ; Phone Mute 
HKR, Settings, "3Jack", 1, 03 ; Use Stereo Mode
HKR, Settings, "20db", 1, 01; Enable Mic 20db Gain by Default.
HKR, Settings, "StereoMic", 1, 01; 0=disable, 1=enable

[SPDIFSpecl.AddReg]
; Enable/Disable the S\PDIF channel
HKR, Disable, "SPDF", 1, 00     ;   01 = Disabled (default), 00 = Enabled
HKR, Disable, "CAC3", 1, 01     ;   00 = AC3 control is shown (default), 01 = AC3 control is not shown
HKR, Disable, "CPCM", 1, 01     ;   00 = PCM control is shown (default), 01 = PCM control is not shown
; S/PDIF channel Data Type
HKR, Settings, "CAC3",  1, 01   ;   00 = AC3 not checked (default), 01 = AC3 checked
HKR, Settings, "CPCM",  1, 01   ;   00 = PCM not checked (default), 01 = PCM checked

[JL1_B6T.AddReg]
HKR, Disable,  "HP_V",             1, 01 ; Disable Headphone Volume Control
HKR, Disable,  "MicS",             1, 01 ; Mic In Select

HKR, Settings, "ACDV",             1, 0C ; Analog CD Volume (not digital redbook !)
HKR, Settings, "ACDVMax",          1, 08 ; Analog CD Volume Maximum (not digital redbook !)
HKR, Settings, "HP_M",             1, 01 ; Headphone Mute
HKR, Settings, "HP_V",             1, 04 ; Headphone Volume
HKR, Settings, "JackSenseDisable", 1, 01 ; Disable Jack Sense circuitry
HKR, Settings, "LinV",             1, 0C ; LineIn Volume
HKR, Settings, "LinVMax",          1, 08 ; LineIn Volume Maximum
HKR, Settings, "MicR",             1, 07 ; Mic Recording level
HKR, Settings, "MicV",             1, 0C ; Mic In Volume
HKR, Settings, "OutR",             1, 01 ; Line output loopback
HKR, Settings, "P3DM",             1, 01 ; Phat 3D Mute
HKR, Settings, "PCMOutVolume",     1, 08 ; PCM Out volume 8 = 0db gain, 7 = +1.5db

[B7_M7.AddReg]
HKR, Settings, "EnableRecordMuting", 1, 01 ; Mute Record when slider at bottom.
HKR, Settings, "HPWithMaster",       1, 01 ; 00 = Normal, 01 = Amplifier output tracks Master
HKR, Settings, "MagicNumber",        1, 00, 30, 00, 60
HKR, Settings, "MicBoostVal",        1, 12 ; AD1981A Microphone Boost. 00 = +20db, 01 = +10db, 02 = +30db.
HKR, Settings, "MicVMax",            1, 00 ; Mic In Volume Maximum
HKR, Settings, "PowerManagement",    1, 01 ; Enable Capture/Playback power management
HKR, Settings, "StereoMic",          1, 01 ; 00 = mono mic support, 01 = stereo mic support
HKR, Settings, "TestReg",            1, 01 ; Enable PLL TestMode. 00 = disable, 01 = enable
HKR, Settings, "VRefDisable",        1, 00 ; AD1981A VRefDisable. 00 = enable, 01 = disable
HKR, Settings, "VRefLevel",          1, 01 ; AD1981A VRefLevel. 00 = 2.25v, 01 = 3.7v
HKR, Settings, "FntVMax", 1, 08   ;   Front Volume
HKR, Settings, "MasV", 1, 05     ;   Master Volume
HKR, Settings, "VidM", 1, 01     ;   Video Volume
HKR, Settings, "ACDM", 1, 00     ;   Analog CD Mute
HKR, Settings, "MonM", 1, 01     ;   Mono Out Mute
HKR, Settings, "FntM", 1, 00     ;   Surround Mute
HKR, Settings, "SurM", 1, 00     ;   Surround Mute
HKR, Settings, "CtrV", 1, 08     ;   Center Volume
HKR, Settings, "CtrM", 1, 00     ;   Center Mute
HKR, Settings, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )
HKR, Settings, "JStr", 1, 01     ;   Use OEM supplied string
HKR, Settings, "NoCopyLeftToRight", 1, 01 ; No Copy (0= copy, 1=no copy)
 
HKR, Disable, "PhoV", 1, 01     ;   Phone Volume
HKR, Disable, "PhoM", 1, 01     ;   Phone Mute
HKR, Disable, "LinM", 1, 00     ;   LineIn Mute
HKR, Disable, "VidV", 1, 01     ;   Video Volume
HKR, Disable, "VidM", 1, 01     ;   Video Mute
HKR, Disable, "LinV", 1, 00     ;   LineIn Volume
HKR, Disable, "LinR", 1, 00     ;   Line In
HKR, Disable, "ACDV", 1, 00     ;   Analog CD Volume (not digital redbook !)
HKR, Disable, "ACDM", 1, 00     ;   Analog CD Mute
HKR, Disable, "MonV", 1, 01     ;   Mono Out Volume
HKR, Disable, "MonM", 1, 01     ;   Mono Out Mute
HKR, Disable, "FntV", 1, 00     ;   Front Volume
HKR, Disable, "FntM", 1, 00     ;   Front Mute
HKR, Disable, "SurV", 1, 00     ;   Surround Volume
HKR, Disable, "SurM", 1, 00     ;   Surround Mute
HKR, Disable, "CtrV", 1, 00     ;   Center Volume
HKR, Disable, "CtrM", 1, 00     ;   Center Mute
HKR, Disable, "LfeV", 1, 00     ;   Lfe Volume ( sub woofer )
HKR, Disable, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )
HKR, Disable, "ACDR", 1, 00     ;   CD (Analog CD, not Redbook Audio)
HKR, Disable, "VidR", 1, 01     ;   Video
HKR, Disable, "MonR", 1, 01     ;   Mono output loopback
HKR, Disable, "PhoR", 1, 01     ;   Phone

[Cbr.AddReg]
HKR, Settings, "Coefficients", 1, \
3c, 22, ac, a0, bc, 46, 08, d7, 54, 5f, \
c9, 39, 58, ab, ef, 3d, 47, c8, a8, 54, \
62, 26, 25, d7, 61, 44, 3d, d5, db, 28, \
5f, 25, af, 3a, 78, 3e, 29, dc, 51, c5, \
b5, 25, c5, 64, 5d, 47, ed, d2, 3b, 9b, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
6d, 29, da, 96, 1c, 45, 77, d1, 26, 69, \
69, 3b, 61, 99, 7a, 3e, 1d, c6, 9f, 66, \
a1, 2c, 87, b6, 50, 43, 0f, d0, 79, 49, \
a5, 2b, a8, 02, d4, 3e, 86, d5, 58, fd, \
33, 2c, c8, 2e, 8c, 45, 41, ce, 38, d1, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
0d, 2b, d0, 94, be, 44, 35, d0, 30, 6b, \
c5, 3b, 08, 96, 98, 3e, a3, c5, f8, 69, \
0a, 2e, 05, b0, 12, 43, e4, ce, fb, 4f, \
13, 2d, b6, f4, e9, 3e, 04, d4, 4a, 0b, \
a8, 2d, b6, 1d, 24, 45, 35, cd, 4a, e2, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
d2, 2f, 34, 8f, a9, 43, 85, cc, cc, 70, \
cb, 3c, b1, 8d, ef, 3e, 46, c4, 4f, 72, \
28, 32, 1d, 9f, 5e, 42, 7a, cb, e3, 60, \
4b, 31, f3, cc, 28, 3f, 8e, cf, 0d, 33, \
e7, 31, 02, e9, f3, 43, 26, ca, fe, 16, \
4e, 80, 00, 00, b2, 7f, 00, 40, 00, 00, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
f5, 33, c6, 8a, ba, 42, 52, c9, 3a, 75, \
a6, 3d, 2a, 88, 38, 3f, 21, c3, d6, 77, \
b7, 35, 46, 93, c2, 41, 87, c8, ba, 6c, \
fd, 34, c1, ae, 5e, 3f, a5, cb, 3f, 51, \
8e, 35, a2, be, ed, 42, 85, c7, 5e, 41, \
af, bc, 3f, 1a, a2, 6b, af, 17, c1, e5, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
df, 34, d9, 89, 85, 42, 9c, c8, 27, 76, \
d6, 3d, 25, 87, 48, 3f, e2, c2, db, 78, \
81, 36, 05, 91, a0, 41, e0, c7, fb, 6e, \
d0, 35, e2, a8, 6a, 3f, c6, ca, 1e, 57, \
5c, 36, 4e, b6, b3, 42, f1, c6, b2, 49, \
78, c6, 6d, 17, 62, 68, 26, 11, 93, e8, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
84, 37, 45, 87, eb, 41, 90, c6, bb, 78, \
5e, 3e, 97, 84, 75, 3f, 2c, c2, 69, 7b, \
c5, 38, 3f, 8b, 3d, 41, fe, c5, c1, 74, \
35, 38, e4, 99, 8d, 3f, 3e, c8, 1c, 66, \
ac, 38, 22, a1, 0d, 42, 46, c5, de, 5e, \
27, e0, 00, 00, d9, 5f, 00, 00, 00, 00, \
00, 00, 00, 00, 00, 40, 00, 00, 00, 00, \
c2, 39, 35, 85, 69, 41, d4, c4, cb, 7a, \
d0, 3e, de, 82, 9b, 3f, 96, c1, 22, 7d, \
b0, 3a, 37, 87, e9, 40, 67, c4, c9, 78, \
3f, 3a, a8, 8f, ab, 3f, 16, c6, 58, 70, \
a0, 3a, fc, 92, 82, 41, df, c3, 04, 6d, \
22, f5, 69, df, e1, 58, fe, f1, 97, 20, \
24, 28, fd, 54, 44, 3d, 98, da, 03, ab, \
40, 3a, c5, 84, 4d, 41, 73, c4, 3b, 7b, \
e8, 3e, 8a, 82, a3, 3f, 75, c1, 76, 7d, \
1b, 3b, 70, 86, d6, 40, 0f, c4, 90, 79, \
b2, 3a, bd, 8d, b2, 3f, 9c, c5, 43, 72, \
0d, 3b, 66, 90, 63, 41, 90, c3, 9a, 6f, \
d6, f9, 6d, d7, 51, 57, da, ee, 93, 28, \
c5, 29, fd, 48, 74, 3d, c8, d8, 03, b7

HKR, Settings, "PM_Max_Power" ,    1, 80
HKR, Settings, "PM_Min_Power" ,    1, 80 ; All sections allowed to power down at min power, except Vref and Mixer.

[Hrr.AddReg]
HKR, Settings, "PhoM",             1, 01 ; Phone Mute

[K1.AddReg]
HKR, Disable, "AuxM",              1, 01 ; Aux Mute
HKR, Disable, "AuxR",              1, 01 ; Aux Recording
HKR, Disable, "AuxV",              1, 01 ; Aux Volume

HKR, Settings, "AuxM",             1, 01 ; Aux Mute
HKR, Settings, "MonoWithMaster",   1, 01 ; 00 = Normal, 01 = MonoOut tracks Master
HKR, Settings, "PhoVMax",          1, 08 ; Phone Volume
HKR, Settings, "PM_Max_Power" ,    1, 80
HKR, Settings, "PM_Min_Power" ,    1, 80

[M1020.ADDREG] 
HKR, Settings, "HP_VMax", 1, 06   ;   Headphone Volume
HKR, Settings, "MicVMax", 1, 02   ;   Mic In Volume
HKR, Settings, "MicVMin", 1, 10   ;
HKR, Settings, "MasV", 1, 08     ;   Master Volume
HKR, Settings, "PCBV", 1, 08     ;   PCBeep Volume
HKR, Settings, "PCBM", 1, 00     ;   PCBeep Mute
HKR, Settings, "MicV", 1, 08     ;   Mic In Volume
HKR, Settings, "ACDV", 1, 08     ;   Analog CD Volume (not digital redbook !)
HKR, Settings, "EnableRecordMuting", 1, 01 ; Mute Record when slider at bottom.
HKR, Settings, "P3DM", 1, 00     ;   Phat 3D Mute
HKR, Settings, "MicBoostVal", 1, 00 ;  AD1981A Microphone Boost. 00 = +20db, 01 = +10db, 02 = +30db
HKR, Settings, "VRefDisable", 1, 00 ;  AD1981A VRefDisable. 00 = enable, 01 = disable
HKR, Settings, "MonoWithMaster", 1, 00 ;   00 = Normal, 01 = MonoOut tracks Master
HKR, Settings, "HP_V", 1, 08     ;   Headphone Volume
HKR, Settings, "OutR", 1, 00
HKR, Disable, "Voice", 1, 01    ;   ICHx MicIn DMA channel. 00 = enable, 01 = disable.
HKR, Disable, "HP_P", 1, 00     ;   Headphone Pin (Headphone destination on AD1885/6)
                                ;    00 = active, 01 = not active

[WDM_AC97AUD_GUID.AddReg]
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Name,,%Pin.PcBeep%
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.Phone%,Name,,%Pin.Phone%
HKLM,%MediaCategories%\%ADIGUID.Phone%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.Video%,Name,,%Pin.Video%
HKLM,%MediaCategories%\%ADIGUID.Video%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Name,,%Pin.MonoOut%
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Name,,%Control.PCBeepVol%
HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Name,,%Control.PhoneVol%
HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Name,,%Control.VIDVol%
HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.20DB%,Name,,%Control.20DB%
HKLM,%MediaCategories%\%ADIGUID.20DB%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Name,,%Control.PHATBypass%
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Name,,%Control.MonoVol%
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Name,,%Control.MicSelect%
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Name,,%Control.CaptureVid%
HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Name,,%Control.CaptureMono%
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Name,,%Control.CapturePhone%
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.Front%,Name,,%Pin.Front%
HKLM,%MediaCategories%\%ADIGUID.Front%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Surround%,Name,,%Pin.Surround%
HKLM,%MediaCategories%\%ADIGUID.Surround%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Center%,Name,,%Pin.Center%
HKLM,%MediaCategories%\%ADIGUID.Center%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Lfe%,Name,,%Pin.Lfe%
HKLM,%MediaCategories%\%ADIGUID.Lfe%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.FrontVol%,Name,,%Control.FrontVol%
HKLM,%MediaCategories%\%ADIGUID.FrontVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SurroundVol%,Name,,%Control.SurroundVol%
HKLM,%MediaCategories%\%ADIGUID.SurroundVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CenterVol%,Name,,%Control.CenterVol%
HKLM,%MediaCategories%\%ADIGUID.CenterVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.LfeVol%,Name,,%Control.LfeVol%
HKLM,%MediaCategories%\%ADIGUID.LfeVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SwapC%,Name,,%Control.SwapC%
HKLM,%MediaCategories%\%ADIGUID.SwapC%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SwapD%,Name,,%Control.SwapD%
HKLM,%MediaCategories%\%ADIGUID.SwapD%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.CAC3%,Name,,%Control.CAC3%
HKLM,%MediaCategories%\%ADIGUID.CAC3%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CPCM%,Name,,%Control.CPCM%
HKLM,%MediaCategories%\%ADIGUID.CPCM%,Display,1,00,00,00,00

[DriverInfo.DelReg]
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%

[DriverInfo.AddReg]
; This section is added to all INFs to add registry entries for Driver Information.
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, DriverBuildDate,,%DriverBuildDate%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileName,,"smwdm.sys"
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileVersion,,"5.12.5410"
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, INFVersion,,%INFVersionID%

[SourceDisksNames]
222=%Empty%,,,

[SourceDisksFiles]
smwdm.sys=222
;; copy these files into the
;; system32\drivers directory

[WDM_AC97AUD.CopyList]
smwdm.sys

;;**************** AMD64 NT Install ****************

[WDM_XPE.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, AusCom.AddReg, AusSiS.AddReg, LinVCom.AddReg, DriverInfo.AddReg

[WDM_ODMSPDFN.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, Odm.AddReg, OdmCom.AddReg, OdmSiS.AddReg, ODMSiS_M.AddReg, LinVCom.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_A188.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, ODMSiS_M.AddReg, OdmFVMax.AddReg, OdA18.AddReg, AusCom.AddReg, OdmSiS.AddReg, A188.AddReg, LinVCom.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_ODMNOSPF.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, ODMSiS_M.AddReg, OdmFVMax.AddReg, Odm.AddReg, AusCom.AddReg, OdmSiS.AddReg, LinVCom.AddReg, M1020.ADDREG

[WDM_Z94L.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, AusCom.AddReg, OdmSiS.AddReg, Z94L.AddReg, M1020.ADDREG

[WDM_ASUS.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, ODMSiS_M.AddReg, Odm.AddReg, AusSiS.AddReg, Js_Je.AddReg, Js_JeA.AddReg, Js_JeB.AddReg, LinVCom.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_SF3.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, ODMSiS_M.AddReg, P4Com.AddReg, Odm8S.AddReg, Sf3Com.AddReg, Sf3.AddReg, LinVCom.AddReg, M1020.ADDREG

[WDM_SF3LEN.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, ODMSiS_M.AddReg, P4Com.AddReg, Sf3Com.AddReg, Sf3Len.AddReg, LinVCom.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_VM5.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, ODMSiS_M.AddReg, AusCom.AddReg, OdmSiS.AddReg, P4Com.AddReg, VM5.AddReg, LinVCom.AddReg, M1020.ADDREG

[WDM_M188.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT,WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, ODMSiS_M.AddReg, OdA18.AddReg, ODMFVM2.AddReg,A188M.AddReg,M188.AddReg,M533.AddReg,SPDIFOff.AddReg, AusCom.AddReg, OdmSiS.AddReg, LinVCom.AddReg, M1020.ADDREG

[WDM_A1986A.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, ODMSiS_M.AddReg, Odm.AddReg, AusSiS.AddReg, Js_Jesis.AddReg, Js_JeA.AddReg, LinVCom.AddReg, ODMSiS_A.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_M939.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, M939.ADDREG, OdmFVMax.AddReg, Sf3Com.AddReg, Sf3Len.AddReg, SPDIFLAP.AddReg, LinVCom.AddReg, M1020.ADDREG

[WDM_CPAL188.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg,ODMSiS_M.AddReg,CPAL188.AddReg, OdmFVMax.AddReg, AusCom.AddReg, OdmSiS.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_T19.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, OdmFVMax.AddReg, AusCom.AddReg, OdmSiS.AddReg, Z94L.AddReg, SPDIFLAP.AddReg, M1020.ADDREG

[WDM_M1981B.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT,WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, ODMFVM2.AddReg,A188M.AddReg, SPDIFOff.AddReg, AusCom.AddReg, OdmSiS.AddReg, LinVCom.AddReg, M1981B.AddReg, M1020.ADDREG

[WDM_HRR.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, SPDIFSpecl.AddReg, JL1_B6T.AddReg, B7_M7.AddReg, Cbr.AddReg, Hrr.AddReg

[WDM_K1.NTamd64]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUDAddReg.NT, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, JL1_B6T.AddReg, B7_M7.AddReg, K1.AddReg

[WDM_XPE.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_ODMSPDFN.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_A188.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_SF3LEN.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_SF3.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_M939.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_CPAL188.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_T19.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_M1981B.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_HRR.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_K1.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_M188.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_ODMNOSPF.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_Z94L.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_VM5.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_A1986A.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

[WDM_ASUS.NTamd64.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology

;;**************** AMD64 NT Install ****************

[AC97Aud.Interface.Wave]
AddReg=AC97Aud.Interface.Wave.AddReg
[AC97Aud.Interface.Wave.AddReg]
HKR,,FriendlyName,,%AC97Aud.Wave.szPname%
HKR,,CLSID,,%Proxy.CLSID%

[AC97Aud.Interface.Topology]
AddReg=AC97Aud.Interface.Topo.AddReg
;;must use topo because topology is too long
[AC97Aud.Interface.Topo.AddReg]
HKR,,FriendlyName,,%AC97Aud.Topology.szPname%

[WDM_XPE.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_ODMSPDFN.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_A188.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_M188.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_SF3LEN.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_ASUS.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_ODMNOSPF.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_Z94L.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_SF3.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_VM5.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_A1986A.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_M939.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_CPAL188.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_T19.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_M1981B.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_HRR.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_K1.NTamd64.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst

[WDM_AC97AUD_Service_Inst]
;DisplayName    = %WDM_AC97AUD.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\system32\drivers\smwdm.sys

[Strings]
;; AC'97 Device friendly names (GUIDS non-localizeable)

ADIGUID.PcBeep      ="{992C6360-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoOut     ="{992C6361-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Phone       ="{992C6362-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Video       ="{992C6366-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PCBeepVol   ="{992C6372-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoVol     ="{992C6374-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PhoneVol    ="{992C6376-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.VIDVol      ="{992C637A-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.20DB        ="{992C6380-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PHATBypass  ="{992C6387-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MicSelect   ="{992C638D-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.CaptureVid  ="{992C6392-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CaptureMono ="{992C6396-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CapturePhone ="{992C6397-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.Front       ="{992C636A-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Surround    ="{992C6365-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Center      ="{992C6364-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Lfe         ="{992C6363-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.FrontVol    ="{992C6370-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.SurroundVol ="{992C6381-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CenterVol   ="{992C6382-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.LfeVol      ="{992C6383-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.SwapC       ="{A3156CDD-A925-4A37-BD1F-BC9D627F3F06}"
ADIGUID.SwapD       ="{A3156CDE-A925-4A37-BD1F-BC9D627F3F06}"

ADIGUID.CAC3        ="{A3156CD9-A925-4A37-BD1F-BC9D627F3F06}"
ADIGUID.CPCM        ="{A3156CDA-A925-4A37-BD1F-BC9D627F3F06}"

;; Analog Devices friendly names (localizeable)
;Sources (Pins)
Pin.PcBeep       ="PC Beep"          ; PC Beep Input
Pin.MonoOut      ="Mono Out"         ; Mono line output
Pin.Phone        ="Phone"            ; Phone Input
Pin.Video        ="Video"            ; Video Input
Pin.Front        ="Front"            ; Front Output
Pin.Surround     ="Rear"             ; Surround Output
Pin.Center       ="Center"           ; Center Channel Output
Pin.Lfe          ="Subwoofer"        ; Sub woofer ( Lfe )

;Controls       (Controls as related to Sources)

Control.PCBeepVol     ="PCBeep Volume"   ; PC Beep volume control name
Control.PhoneVol      ="Phone Volume"    ; Phone volume control name
Control.VIDVol        ="Video Volume"    ; Video volume control name
Control.20DB          ="MIC Boost"       ; Microphone advanced control
Control.PHATBypass    ="Apply 3D effect to digital audio"
                                         ; 3D bypass control string (bypass
                                         ;  spatialization on digital streams)

Control.MonoVol       ="Mono Volume"     ; Monoaural Output volume control name
Control.MicSelect     ="Front Panel Microphone" ; Microphone advanced control

Control.CaptureVid    ="Video"           ; Video Record
Control.CaptureMono   ="Mono Out"        ; Mono Mix Record
Control.CapturePhone  ="Phone"           ; Phone Record

Control.FrontVol     ="Front Volume"     ; Front Output
Control.SurroundVol  ="Rear Volume"      ; Surround Output
Control.CenterVol    ="Center Volume"    ; Center Channel Output
Control.LfeVol       ="Subwoofer Volume" ; Sub woofer ( Lfe )
Control.SwapC        ="Swap Center/Subwoofer"
Control.SwapD        ="Swap Center/Subwoofer Data"

Control.CAC3	     ="AC3 SPDIF"	 ; AC3 Select
Control.CPCM	     ="PCM SPDIF"	 ; PCM Select

MediaCategories="SYSTEM\CurrentControlSet\Control\MediaCategories"
WDM_MIDI="WDM-based Device"
Proxy.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO="{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSNAME_Wave="Wave"
KSNAME_Topology="Topology"

ANLG="Analog Devices"
MfgName="Analog Devices, Inc."
Empty="Install disk"

*WDM_AC97AUD.DeviceDesc="(PE64) SoundMAX Integrated Digital Audio"
AC97Aud.Wave.szPname="SoundMAX Digital Audio"
AC97Aud.Topology.szPname="SoundMAX Digital Audio"

; History Information
DriverMfgr="AnalogDevices"
DriverVersionID="5.12.5500"
DriverBuildDate="05/29/2007"
DriverBuildID="5.12.02.5500"
INFVersionID="5.12.02.5500-0000"
DriverNatUp="2.710-66.192230"
DriverOEM="AnalogDevices"
DriverFamily="Audio"
DriverProduct="SoundMAX"
DriverDescription="Audio Driver"
DriverOEMVersion="x00"

