
       Оптимизированный драйвер INTEL Graphics 10.18.10.3379 для использования в PE_7x64, PE_8x64.

    Драйвер пригоден для установщика DevInst, SDI или стандартного обновления устройств.

    Для стандартного обновления устройств распакуйте драйвер до уровня каталогов с файлами.

--------------------------------------------------------------------------------------------------

      Драйвер INTEL Graphics 10.18.10.3379 Windows 7/8 (64 bit), каталог IG1018103379_NT6x64.     

    DriverVer=12/20/2013, 10.18.10.3379. Отключены OpenCL, OpenGL, ControlPanel. Product Support:

    Supports Intel(R) Iris(TM) graphics, Intel(R) Iris(TM) Pro graphics, Intel(R) HD graphics,
    Intel(R) Bay Trail -M/D SOC HD Graphics on: 

    5th Generation Intel(R) Broadwell Processor Family
    Bay Trail Processor Family
    4th Generation Intel(R) Core(TM) Processor Platform
    4th Generation Intel(R) Core(TM) Processor U Series based Platform
    3rd Generation Intel(R) Core(TM) Processor Platform
    3rd Generation Intel(R) Core(TM) Processor U Series based Platform
    3rd Generation Intel(R) Core(TM) Processor Y Series based Platform
    Intel(R) Pentium(R) Processor 2000/3000/G2000/G2100/G3000 Series 
    Intel(R) Celeron(R) Processor 900/1000/2000/G1000 Series
    Intel(R) Pentium(R) N3510/ 3520 Processor 
    Intel(R) Celeron(R) N2810/ 2820 Processor 
    Intel(R) Celeron(R) N2910/ 2920 Processor 
    Intel(R) Celeron(R) N2805/ N2806 Processor
    Intel(R) Celeron(R) N2815 Processor
    Intel(R) Pentium(R) J2850/ J2900 Processor
    Intel(R) Celeron(R) J1850/ J1900 Processor
    Intel(R) Celeron(R) J1750/ J1800 Processor  
    Intel(R) Celeron(R) Pentium QC (N3520)1 
    Intel(R) Celeron(R)  QC  (N2920)1 
    Intel(R) Celeron(R)  DC  (N2820)1 
    Intel(R) Celeron(R)  DC  (N2806)1 
    Intel(R) Celeron(R)  DC  (N2815)1 
    Intel(R) Celeron(R)  QC (J2900)1 
    Intel(R) Celeron(R)  QC  (J1900)1 
    Intel(R) Celeron(R)  DC  (J1800)

--------------------------------------------------------------------------------------------------

    ; 3rd Generation Intel® IvyBridge HD Graphics
    iIVBGD0       = "(PE64) Intel(R) 3rd Generation IvyBridge HD Graphics 4000"
    iIVBGM0       = "(PE64) Intel(R) 3rd Generation IvyBridge HD Graphics 4000"
    iIVBGD0SRV    = "(PE64) Intel(R) 3rd Generation IvyBridge HD Graphics P4000"
    iIVBGD0GT1    = "(PE64) Intel(R) 3rd Generation IvyBridge HD Graphics GT1"
    iIVBGM0GT1    = "(PE64) Intel(R) 3rd Generation IvyBridge HD Graphics GT1"
    iIVBGD0SRVGT1 = "(PE64) Intel(R) 3rd Generation IvyBridge HD / Server Graphics GT1"

    ; Intel chipsets/processors (formerly Bay Trail -M/D SOC)
    iVLVGMT0    = "(PE64) Intel(R) Bay Trail HD Graphics"

    ; HSW A0/A1 4th Generation Intel(R) Haswell HD Graphics
    iHSWGTLD    = "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTL"
    iHSWGTLM    = "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTL"
    iHSWGTMD   	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTM"
    iHSWGTMM   	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTM"
    iHSWGTHD   	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTH"
    iHSWGTHM   	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics - GTH"

    ; HSW Classic 4th Generation Intel(R) Haswell HD Graphics
    iHSWGT1D   	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWGT1M    = "(PE64) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWGT15D   = "(PE64) Intel(R) 4th Generation Haswell HD Graphics 4400"
    iHSWGT2D    = "(PE64) Intel(R) 4th Generation Haswell HD Graphics 4600"
    iHSWGT2M    = "(PE64) Intel(R) 4th Generation Haswell HD Graphics 4600"

    ; HSW ULT 4th Generation Intel(R) Haswell HD Graphics
    iHSWGT1UT   = "(PE64) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWGT2UT   = "(PE64) Intel(R) 4th Generation Haswell HD Graphics Family"
    iHSWGT3UT   = "(PE64) Intel(R) 4th Generation Haswell HD Graphics 5000"
    iHSWGT3UT25W= "(PE64) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5100"
    iHSWGT2UX   = "(PE64) Intel(R) 4th Generation Haswell HD Graphics Family"
    iHSWGT1ULX	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics"

    ; HSW CRW 4th Generation Intel(R) Haswell HD Graphics
    iHSWGT2CW  	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics 4600"
    iHSWGT2CWDT = "(PE64) Intel(R) 4th Generation Haswell HD Graphics 4600"
    iHSWGT3CW  	= "(PE64) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5200 with High Speed Memory"
    iHSWGT3CWDT = "(PE64) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5200 with High Speed Memory"

    ; HSW SRVR 4th Generation Intel(R) Haswell HD Graphics
    iHSWSVGT1  	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWSVGT2  	= "(PE64) Intel(R) 4th Generation Haswell HD Graphics P4600/P4700"

    ; BDW Simulation 5th Generation Intel(R) Broadwell HD Graphics
    iBDWGD0     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS"
    iBDWGT0     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS GT0"
    iBDWGT1     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS GT1"
    iBDWGT2     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS GT2"
    iBDWGT3     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS GT3"
    iBDWGT4     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics HAS GT4"

    ; BDW HW 5th Generation Intel(R) Broadwell HD Graphics
    iBDWMULTGT1 = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics M ULT GT1"
    iBDWULXGT1  = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics ULX GT1"
    iBDWMULTGT2 = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics M ULT GT2"
    iBDWULXGT2  = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics ULX GT2"
    iBWDHALOGT1 = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics Halo GT1"
    iBWDHALOGT2 = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics Halo GT2"
    iBWDHALOGT3 = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics Halo GT3"

--------------------------------------------------------------------------------------------------

      В случае установки драйвера  видеоадаптера  через диспетчер устройств,  необходимо выполнить

    детект PnP устройств или запустить утилиту типа Resolution Changer SX2 для того чтобы заменить

    пока еще работающий стандартный VGA драйвер  (иначе появляется ошибка при изменении параметров

    экрана).  При подключении  посредством  DevInst.exe автоматически  устанавливается оптимальное

    разрешение и частота регенерации для обнаруженного типа монитора.

==================================================================================================
 29-Jan-2017 nat27 http://forum.ru-board.com/topic.cgi?forum=62&topic=24098&start=71&limit=1&m=1#1
==================================================================================================
  