
;=============================================================================
;
; Copyright (c) Intel Corporation (2013).
;
; INTEL MAKES NO WARRANTY OF ANY KIND REGARDING THE CODE.  THIS CODE IS
; LICENSED ON AN "AS IS" BASIS AND INTEL WILL NOT PROVIDE ANY SUPPORT,
; ASSISTANCE, INSTALLATION, TRAINING OR OTHER SERVICES.  INTEL DOES NOT
; PROVIDE ANY UPDATES, ENHANCEMENTS OR EXTENSIONS.  INTEL SPECIFICALLY
; DISCLAIMS ANY WARRANTY OF MERCHANTABILITY, NONINFRINGEMENT, FITNESS FOR ANY
; PARTICULAR PURPOSE, OR ANY OTHER WARRANTY.  Intel disclaims all liability,
; including liability for infringement of any proprietary rights, relating to
; use of the code. No license, express or implied, by estoppel or otherwise,
; to any intellectual property rights is granted herein.
;
;=============================================================================

;
; Installation inf for the Intel Corporation graphics adapter.
;
[Version]
Signature="$WINDOWS NT$"
Provider=%Intel%
ClassGUID={4D36E968-E325-11CE-BFC1-08002BE10318}
Class=Display
CatalogFile=igdlh.cat
DriverVer=12/20/2013,10.18.10.3379

; nat27 prepared for NT6x86_PE 06-Jan-2014, mod 31-Jan-2017
; original inf DriverVer=11/12/2013,9.17.10.3353
; Video_IN3_x86(1702)

[SignatureAttributes]
igdumdim32.dll=SignatureAttributes.PETrust
igd10iumd32.dll=SignatureAttributes.PETrust
igdusc32.dll=SignatureAttributes.PETrust

[SignatureAttributes.PETrust]
PETrust=true

[DestinationDirs]
DefaultDestDir  = 11  ; system32
igfx.Miniport   = 12  ; drivers
igfx.UserMode   = 11  ; system32
IMOLA9.Copy     = 11  ; system32

;
; Driver information
;
[Manufacturer]
%Intel%   = IntelGfx, NTx86.6.1, NTx86.6.2, NTx86.6.3

;=====================================================================
;    Windows 7 Install
;=====================================================================
[IntelGfx.NTx86.6.1]
; HSW A0/A1
%iHSWGTLD%   	= iHSWD_w7, PCI\VEN_8086&DEV_0C02
%iHSWGTLM%    	= iHSWM_w7, PCI\VEN_8086&DEV_0C06
%iHSWGTMD%    	= iHSWD_w7, PCI\VEN_8086&DEV_0C12
%iHSWGTMM%    	= iHSWM_w7, PCI\VEN_8086&DEV_0C16
%iHSWGTHD%    	= iHSWD_w7, PCI\VEN_8086&DEV_0C22
%iHSWGTHM%    	= iHSWM_w7, PCI\VEN_8086&DEV_0C26
; HSW
%iHSWGT1D%   	= iHSWD_w7, PCI\VEN_8086&DEV_0402
%iHSWGT1M%    	= iHSWM_w7, PCI\VEN_8086&DEV_0406
%iHSWGT2D%   	= iHSWD_w7, PCI\VEN_8086&DEV_0412
%iHSWGT2M%    	= iHSWM_w7, PCI\VEN_8086&DEV_0416
%iHSWGT15D%    	= iHSWD_w7, PCI\VEN_8086&DEV_041E
; HSW ULT
%iHSWGT1UT%    	= iHSWM_w7, PCI\VEN_8086&DEV_0A06
%iHSWGT2UT%    	= iHSWM_w7, PCI\VEN_8086&DEV_0A16
%iHSWGT3UT%    	= iHSWM_w7, PCI\VEN_8086&DEV_0A26
%iHSWGT3UT25W%  = iHSWM_w7, PCI\VEN_8086&DEV_0A2E
%iHSWGT2UX%  	= iHSWM_w7, PCI\VEN_8086&DEV_0A1E
%iHSWGT1ULX%  	= iHSWM_w7, PCI\VEN_8086&DEV_0A0E
; HSW CRW
%iHSWGT2CW%    	= iHSWM_w7, PCI\VEN_8086&DEV_0D16
%iHSWGT3CW%    	= iHSWM_w7, PCI\VEN_8086&DEV_0D26
%iHSWGT2CWDT%   = iHSWD_w7, PCI\VEN_8086&DEV_0D12
%iHSWGT3CWDT%   = iHSWD_w7, PCI\VEN_8086&DEV_0D22
; HSW Server
%iHSWSVGT1%   	= iHSWD_w7, PCI\VEN_8086&DEV_040A
%iHSWSVGT2%    	= iHSWD_w7, PCI\VEN_8086&DEV_041A
; BDW Simulation
%iBDWGD0%       = iBDWM_w7, PCI\VEN_8086&DEV_0090
%iBDWGT0%    	= iBDWM_w7, PCI\VEN_8086&DEV_0BD0
%iBDWGT1%   	= iBDWM_w7, PCI\VEN_8086&DEV_0BD1
%iBDWGT2%   	= iBDWM_w7, PCI\VEN_8086&DEV_0BD2
%iBDWGT3%   	= iBDWM_w7, PCI\VEN_8086&DEV_0BD3	
%iBDWGT4%   	= iBDWM_w7, PCI\VEN_8086&DEV_0BD4
; BDW HW
%iBDWMULTGT1%	= iBDWM_w7, PCI\VEN_8086&DEV_1602
%iBDWMULTGT1%	= iBDWM_w7, PCI\VEN_8086&DEV_1606
%iBDWULXGT1%	= iBDWM_w7, PCI\VEN_8086&DEV_160E
%iBDWMULTGT2%	= iBDWM_w7, PCI\VEN_8086&DEV_1612
%iBDWMULTGT2%	= iBDWM_w7, PCI\VEN_8086&DEV_1616
%iBDWULXGT2%	= iBDWM_w7, PCI\VEN_8086&DEV_161E
%iBWDHALOGT1%   = iBDWM_w7, PCI\VEN_8086&DEV_160B
%iBWDHALOGT2%   = iBDWM_w7, PCI\VEN_8086&DEV_161B
%iBWDHALOGT3%   = iBDWM_w7, PCI\VEN_8086&DEV_162B
;=====================================================================
;    Windows 8 Install
;=====================================================================
[IntelGfx.NTx86.6.2]
; HSW A0/A1
%iHSWGTLD%   	= iHSWD_w8, PCI\VEN_8086&DEV_0C02
%iHSWGTLM%    	= iHSWM_w8, PCI\VEN_8086&DEV_0C06
%iHSWGTMD%    	= iHSWD_w8, PCI\VEN_8086&DEV_0C12
%iHSWGTMM%    	= iHSWM_w8, PCI\VEN_8086&DEV_0C16
%iHSWGTHD%    	= iHSWD_w8, PCI\VEN_8086&DEV_0C22
%iHSWGTHM%    	= iHSWM_w8, PCI\VEN_8086&DEV_0C26
; HSW
%iHSWGT1D%   	= iHSWD_w8, PCI\VEN_8086&DEV_0402
%iHSWGT1M%    	= iHSWM_w8, PCI\VEN_8086&DEV_0406
%iHSWGT2D%   	= iHSWD_w8, PCI\VEN_8086&DEV_0412
%iHSWGT2M%    	= iHSWM_w8, PCI\VEN_8086&DEV_0416
%iHSWGT15D%    	= iHSWD_w8, PCI\VEN_8086&DEV_041E
; HSW ULT
%iHSWGT1UT%    	= iHSWM_w8, PCI\VEN_8086&DEV_0A06
%iHSWGT2UT%    	= iHSWM_w8, PCI\VEN_8086&DEV_0A16
%iHSWGT3UT%    	= iHSWM_w8, PCI\VEN_8086&DEV_0A26
%iHSWGT3UT25W%  = iHSWM_w8, PCI\VEN_8086&DEV_0A2E
%iHSWGT2UX%  	= iHSWM_w8, PCI\VEN_8086&DEV_0A1E
%iHSWGT1ULX%  	= iHSWM_w8, PCI\VEN_8086&DEV_0A0E
; HSW CRW
%iHSWGT2CW%    	= iHSWM_w8, PCI\VEN_8086&DEV_0D16
%iHSWGT3CW%    	= iHSWM_w8, PCI\VEN_8086&DEV_0D26
%iHSWGT2CWDT%   = iHSWD_w8, PCI\VEN_8086&DEV_0D12
%iHSWGT3CWDT%   = iHSWD_w8, PCI\VEN_8086&DEV_0D22
; HSW Server
%iHSWSVGT1%   	= iHSWD_w8, PCI\VEN_8086&DEV_040A
%iHSWSVGT2%    	= iHSWD_w8, PCI\VEN_8086&DEV_041A
; BDW Simulation
%iBDWGD0%       = iBDWM_w8, PCI\VEN_8086&DEV_0090
%iBDWGT0%    	= iBDWM_w8, PCI\VEN_8086&DEV_0BD0
%iBDWGT1%   	= iBDWM_w8, PCI\VEN_8086&DEV_0BD1
%iBDWGT2%   	= iBDWM_w8, PCI\VEN_8086&DEV_0BD2
%iBDWGT3%   	= iBDWM_w8, PCI\VEN_8086&DEV_0BD3	
%iBDWGT4%   	= iBDWM_w8, PCI\VEN_8086&DEV_0BD4
; BDW HW
%iBDWMULTGT1%	= iBDWM_w8, PCI\VEN_8086&DEV_1602
%iBDWMULTGT1%	= iBDWM_w8, PCI\VEN_8086&DEV_1606
%iBDWULXGT1%	= iBDWM_w8, PCI\VEN_8086&DEV_160E
%iBDWMULTGT2%	= iBDWM_w8, PCI\VEN_8086&DEV_1612
%iBDWMULTGT2%	= iBDWM_w8, PCI\VEN_8086&DEV_1616
%iBDWULXGT2%	= iBDWM_w8, PCI\VEN_8086&DEV_161E
%iBWDHALOGT1%   = iBDWM_w8, PCI\VEN_8086&DEV_160B
%iBWDHALOGT2%   = iBDWM_w8, PCI\VEN_8086&DEV_161B
%iBWDHALOGT3%   = iBDWM_w8, PCI\VEN_8086&DEV_162B
;=====================================================================
;    Windows Blue Install ( Uses Win8 sections )
;=====================================================================
[IntelGfx.NTx86.6.3]
; HSW A0/A1
%iHSWGTLD%   	= iHSWD_w81, PCI\VEN_8086&DEV_0C02
%iHSWGTLM%    	= iHSWM_w81, PCI\VEN_8086&DEV_0C06
%iHSWGTMD%    	= iHSWD_w81, PCI\VEN_8086&DEV_0C12
%iHSWGTMM%    	= iHSWM_w81, PCI\VEN_8086&DEV_0C16
%iHSWGTHD%    	= iHSWD_w81, PCI\VEN_8086&DEV_0C22
%iHSWGTHM%    	= iHSWM_w81, PCI\VEN_8086&DEV_0C26
; HSW
%iHSWGT1D%   	= iHSWD_w81, PCI\VEN_8086&DEV_0402
%iHSWGT1M%    	= iHSWM_w81, PCI\VEN_8086&DEV_0406
%iHSWGT2D%   	= iHSWD_w81, PCI\VEN_8086&DEV_0412
%iHSWGT2M%    	= iHSWM_w81, PCI\VEN_8086&DEV_0416
%iHSWGT15D%    	= iHSWD_w81, PCI\VEN_8086&DEV_041E
; HSW ULT
%iHSWGT1UT%    	= iHSWM_w81, PCI\VEN_8086&DEV_0A06
%iHSWGT2UT%    	= iHSWM_w81, PCI\VEN_8086&DEV_0A16
%iHSWGT3UT%    	= iHSWM_w81, PCI\VEN_8086&DEV_0A26
%iHSWGT3UT25W%  = iHSWM_w81, PCI\VEN_8086&DEV_0A2E
%iHSWGT2UX%  	= iHSWM_w81, PCI\VEN_8086&DEV_0A1E
%iHSWGT1ULX%  	= iHSWM_w81, PCI\VEN_8086&DEV_0A0E
; HSW CRW
%iHSWGT2CW%     = iHSWM_w81, PCI\VEN_8086&DEV_0D16
%iHSWGT3CW%     = iHSWM_w81, PCI\VEN_8086&DEV_0D26
%iHSWGT2CWDT%   = iHSWD_w81, PCI\VEN_8086&DEV_0D12
%iHSWGT3CWDT%   = iHSWD_w81, PCI\VEN_8086&DEV_0D22
; HSW Server
%iHSWSVGT1%   	= iHSWD_w81, PCI\VEN_8086&DEV_040A
%iHSWSVGT2%    	= iHSWD_w81, PCI\VEN_8086&DEV_041A
; BDW Simulation
%iBDWGD0%       = iBDWM_w81, PCI\VEN_8086&DEV_0090
%iBDWGT0%    	= iBDWM_w81, PCI\VEN_8086&DEV_0BD0
%iBDWGT1%   	= iBDWM_w81, PCI\VEN_8086&DEV_0BD1
%iBDWGT2%   	= iBDWM_w81, PCI\VEN_8086&DEV_0BD2
%iBDWGT3%   	= iBDWM_w81, PCI\VEN_8086&DEV_0BD3	
%iBDWGT4%   	= iBDWM_w81, PCI\VEN_8086&DEV_0BD4
; BDW HW
%iBDWMULTGT1%	= iBDWM_w81, PCI\VEN_8086&DEV_1602
%iBDWMULTGT1%	= iBDWM_w81, PCI\VEN_8086&DEV_1606
%iBDWULXGT1%	= iBDWM_w81, PCI\VEN_8086&DEV_160E
%iBDWMULTGT2%	= iBDWM_w81, PCI\VEN_8086&DEV_1612
%iBDWMULTGT2%	= iBDWM_w81, PCI\VEN_8086&DEV_1616
%iBDWULXGT2%	= iBDWM_w81, PCI\VEN_8086&DEV_161E
%iBWDHALOGT1%   = iBDWM_w81, PCI\VEN_8086&DEV_160B
%iBWDHALOGT2%   = iBDWM_w81, PCI\VEN_8086&DEV_161B
%iBWDHALOGT3%   = iBDWM_w81, PCI\VEN_8086&DEV_162B
;
; General installation section
;
;=====================================================================
;  Windows 8 Device Sections
;=====================================================================
[iHSWM_w8]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy 
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =  igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg  = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_Mobile_AddSwSettings
DelReg  = Common_Mobile_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
DelReg  = PwrCons_UserPolicy_DelSwSettings
AddReg = PwrCons_HSW_AddSwSettings
AddReg = MediaRRSupport_HSW_AddSwSettings
AddReg = AlternateScramblerSupport_HSW_AddSwSettings
AddReg = DisplayDPP_HSW_AddSwSettings
AddReg = DisplayOptimization_HSW_AddSwSettings
DelReg  = DisplayOptimization_DelSwSettings
AddReg = igfx_SLT_NB_AddSwSettings
DelReg  = igfx_SLT_NB_DelSwSettings
AddReg = EnableDetachableEDPSupport_HSW_AddSwSettings
DelReg  = EnableDetachableEDPSupport_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iHSWM_w8.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWM_w8.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWM_w8.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iHSWD_w8]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy 
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_DT_AddSwSettings
DelReg  = Common_DT_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_HSW_AddSwSettings
AddReg =  MediaRRSupport_HSW_AddSwSettings
AddReg =  AlternateScramblerSupport_HSW_AddSwSettings
AddReg =  DisplayDPP_HSW_AddSwSettings
AddReg =  DisplayOptimization_HSW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings

[iHSWD_w8.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWD_w8.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWD_w8.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iBDWM_w8]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy 
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_Mobile_AddSwSettings
DelReg  = Common_Mobile_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_BDW_AddSwSettings
AddReg =  MediaRRSupport_BDW_AddSwSettings
AddReg =  AlternateScramblerSupport_BDW_AddSwSettings
AddReg =  DisplayDPP_BDW_AddSwSettings
AddReg =  DisplayOptimization_BDW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings
AddReg = EnableDetachableEDPSupport_BDW_AddSwSettings
DelReg  = EnableDetachableEDPSupport_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iBDWM_w8.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iBDWM_w8.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iBDWM_w8.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================

;=====================================================================
;  Windows 8.1 Device Sections
;=====================================================================
[iHSWM_w81]
FeatureScore=DA
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg  = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_Mobile_AddSwSettings
DelReg  = Common_Mobile_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
DelReg  = PwrCons_UserPolicy_DelSwSettings
AddReg = PwrCons_HSW_AddSwSettings
AddReg = MediaRRSupport_HSW_AddSwSettings
AddReg = AlternateScramblerSupport_HSW_AddSwSettings
AddReg = DisplayDPP_HSW_AddSwSettings
AddReg = DisplayOptimization_HSW_AddSwSettings
DelReg  = DisplayOptimization_DelSwSettings
AddReg = igfx_SLT_NB_AddSwSettings
DelReg  = igfx_SLT_NB_DelSwSettings
AddReg = EnableDetachableEDPSupport_HSW_AddSwSettings
DelReg  = EnableDetachableEDPSupport_DelSwSettings

AddReg = igfx_MC_AddSwSettings
DelReg  = igfx_MC_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iHSWM_w81.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWM_w81.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWM_w81.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iHSWD_w81]
FeatureScore=DA
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_DT_AddSwSettings
DelReg  = Common_DT_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_HSW_AddSwSettings
AddReg =  MediaRRSupport_HSW_AddSwSettings
AddReg =  AlternateScramblerSupport_HSW_AddSwSettings
AddReg =  DisplayDPP_HSW_AddSwSettings
AddReg =  DisplayOptimization_HSW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings

AddReg = igfx_MC_AddSwSettings
DelReg  = igfx_MC_DelSwSettings

[iHSWD_w81.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWD_w81.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWD_w81.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iBDWM_w81]
FeatureScore=DA
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_Mobile_AddSwSettings
DelReg  = Common_Mobile_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_BDW_AddSwSettings
AddReg =  MediaRRSupport_BDW_AddSwSettings
AddReg =  AlternateScramblerSupport_BDW_AddSwSettings
AddReg =  DisplayDPP_BDW_AddSwSettings
AddReg =  DisplayOptimization_BDW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings
AddReg = EnableDetachableEDPSupport_BDW_AddSwSettings
DelReg  = EnableDetachableEDPSupport_DelSwSettings

AddReg = igfx_MC_AddSwSettings
DelReg  = igfx_MC_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iBDWM_w81.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iBDWM_w81.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iBDWM_w81.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================

;=====================================================================
;  Windows 7 Device Sections
;=====================================================================
[iHSWM_w7]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg  = OpenCL.DelReg

AddReg = Common_AddSwSettings
DelReg  = Common_DelSwSettings
AddReg = Common_DT_AddSwSettings
DelReg  = Common_DT_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings
DelReg  = PwrCons_UserPolicy_DelSwSettings		; Delete device specific regkeys
AddReg = PwrCons_HSW_AddSwSettings
AddReg = MediaRRSupport_HSW_AddSwSettings
AddReg = AlternateScramblerSupport_HSW_AddSwSettings
AddReg = DisplayDPP_HSW_AddSwSettings
AddReg = DisplayOptimization_HSW_AddSwSettings
DelReg  = DisplayOptimization_DelSwSettings
AddReg = igfx_SLT_NB_AddSwSettings
DelReg  = igfx_SLT_NB_DelSwSettings
AddReg =  EnableDetachableEDPSupport_HSW_AddSwSettings
DelReg  =  EnableDetachableEDPSupport_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iHSWM_w7.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWM_w7.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWM_w7.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iHSWD_w7]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg =  Common_AddSwSettings
DelReg  =  Common_DelSwSettings
AddReg =  Common_DT_AddSwSettings
DelReg  =  Common_DT_DelSwSettings

DelReg  =  Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_HSW_AddSwSettings
AddReg =  MediaRRSupport_HSW_AddSwSettings
AddReg =  AlternateScramblerSupport_HSW_AddSwSettings
AddReg =  DisplayDPP_HSW_AddSwSettings
AddReg =  DisplayOptimization_HSW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings

[iHSWD_w7.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iHSWD_w7.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iHSWD_w7.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================
[iBDWM_w7]
FeatureScore=E0
CopyFiles=igfx.Miniport, igfx.UserMode, Opm.Copy, IMOLA9.Copy
AddReg =  igfx_SoftwareDX11SettingsImola
AddReg =  igfx_SoftwareCommonSettings
DelReg =   igfx_RemoveDeviceSettings

DelReg  = CUI.DelReg
DelReg  = CUISDK.DelReg

AddReg  = OpenGL.Not_Installed

DelReg = OpenCL.DelReg

AddReg =  Common_AddSwSettings
DelReg  =  Common_DelSwSettings
AddReg =  Common_DT_AddSwSettings
DelReg  =  Common_DT_DelSwSettings

DelReg  = Common_Device_Specific_DelSwSettings		; Delete device specific regkeys
AddReg =  PwrCons_BDW_AddSwSettings
AddReg =  MediaRRSupport_BDW_AddSwSettings
AddReg  = AlternateScramblerSupport_BDW_AddSwSettings
AddReg =  DisplayDPP_BDW_AddSwSettings
AddReg =  DisplayOptimization_BDW_AddSwSettings
DelReg  =  DisplayOptimization_DelSwSettings
AddReg =  igfx_SLT_NB_AddSwSettings
DelReg  =  igfx_SLT_NB_DelSwSettings

AddPowerSetting = PowerPlanSettings

[iBDWM_w7.HW]
AddReg = igfx_MSI_HardwareDeviceSettings

[iBDWM_w7.GeneralConfigData]
MaximumNumberOfDevices = 2
MaximumDeviceMemoryConfiguration = 512

[iBDWM_w7.Services]
AddService = igfx, 0x00000002, igfx_Service_Inst

;=====================================================================

;
; File sections
;

[igfx.Miniport]
igdkmd32.sys

[igfx.UserMode]
igd10iumd32.dll,,,0x00004000  ; COPYFLG_IN_USE_TRY_RENAME
igdusc32.dll,,,0x00004000  ; COPYFLG_IN_USE_TRY_RENAME

[IMOLA9.Copy]
igdumdim32.dll,,,0x00004000  ; COPYFLG_IN_USE_TRY_RENAME

[Opm.Copy]

;=======================================================================

;
; OpenGL Not Installed
;
[OpenGL.Not_Installed]
HKR,,    OpenGLInstalled,        %REG_DWORD%,     0x00      ; Open GL drivers not installed

[OpenCL.DelReg]
HKLM,"SOFTWARE\Khronos\OpenCL\Vendors", igdrcl32.dll

[CUI.DelReg]
HKLM,%CUIDeviceIndependentKey%
; Delete old style cui/driver share key
HKLM,%CUIDriverOldShareKey%
; Delete old style cui keys which are device dependent
HKLM,Software\INTEL\igfxcui
HKR,igfxEM
HKR,igfxHK
HKR,igfxcfg
HKR,igfxcpl
HKR,igfxpph
HKR,igfxsrvc
HKR,igfxtray
HKR,shellex\PropertySheetHandlers
HKR,, Display1_EnableLFPPrimaryInDDC
;
; Service Installation
;
[igfx_Service_Inst]
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3                 ; SERVICE_DEMAND_START
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
LoadOrderGroup = Video
ServiceBinary  = %12%\igdkmd32.sys


;
; DX11 Capable SKUS with Imola driver
;
[igfx_SoftwareDX11SettingsImola]
HKR,, InstalledDisplayDrivers,  %REG_MULTI_SZ%, igdumdim32, igd10iumd32, igd10iumd32
HKR,, UserModeDriverName,       %REG_MULTI_SZ%, igdumdim32.dll, igd10iumd32.dll, igd10iumd32.dll

;
; Common Basic Device Settings
;
[igfx_SoftwareCommonSettings]
HKR,, UserModeDriverGUID,       %REG_SZ%, "{6C4BE3D5-831A-42ED-AA62-2AEB34C8CBA4}"
HKR,, MultifunctionSupported,   %REG_DWORD%,    1
HKR,, VgaCompatible,            %REG_DWORD%,    0
HKR,, NativeResolution,         %REG_DWORD%,    1
HKR,, NativeBPP,                %REG_DWORD%,    1
HKR,, ConfigID,                 %REG_DWORD%,    0
HKR,, PC_Release_Major,         %REG_DWORD%,    15           ;Dummy value
HKR,, PC_Release_Minor,         %REG_DWORD%,    26             ;
HKR,, BIOSHPDSupport,           %REG_DWORD%,    00
HKR,, EnableFakeCRT,            %REG_DWORD%,    01
HKR,, IntelDefaultPers,         %REG_DWORD%,    00
HKR,, ApplyNativeMode,          %REG_DWORD%,    00
HKR,, DelayInPointerShapeChange,%REG_DWORD%,    01

; Overlay specific settings
HKR,, Disable_OverlayDSQualityEnhancement,  %REG_DWORD%,     0

; Rotation specific settings
HKR,,   Display1_EnableRotation,    %REG_DWORD%,    0x1
HKR,,   Display1_RotationCaps,      %REG_DWORD%,    0x7     ;Portrait, Inverted Landscape, Inverted Portrait
HKR,,   Display2_RotationCaps,      %REG_DWORD%,    0x7     ;Portrait, Inverted Landscape, Inverted Portrait
HKR,,   Display1_IndependentRotation,    %REG_DWORD%,    0x00
HKR,,   Display1_EnableIndependentRotation,    %REG_DWORD%,    0x00
HKR,,   Display1_EnableIDDC_WA,               %REG_DWORD%,    0x00
HKR,,   RotationSPLCase,    %REG_DWORD%,    0x00
HKR,,   SmoothRotationSupport,    %REG_DWORD%,    0x00

; Event Manager specific settings
;HKR,,    DisplayPriority,        0x00000001,     0x08, 0x80, 0x01, 0x10, 0x04, 0x40, 0x02, 0x20 ;descending
;HKR,,     EDIDDefaultXX,        %REG_DWORD%,    0x320
;HKR,,    EDIDDefaultYY,        %REG_DWORD%,    0x258
;HKR,,    EDIDDefaultRR,        %REG_DWORD%,    0x3c
;HKR,,    EDIDDefaultBPP,        %REG_DWORD%,    0x20
;HKR,,    LegacyDefaultXX,        %REG_DWORD%,    0x320
;HKR,,    LegacyDefaultYY,        %REG_DWORD%,    0x258
;HKR,,    LegacyDefaultRR,        %REG_DWORD%,    0x3c
;HKR,,    LegacyDefaultBPP,        %REG_DWORD%,    0x20

HKLM,"SYSTEM\CurrentControlSet\Control\GraphicsDrivers",UseXPModel,%REG_DWORD%,0
HKLM,"SYSTEM\CurrentControlSet\Control\GraphicsDrivers\Scheduler",EnablePreemption,%REG_DWORD%,1

[igfx_MSI_HardwareDeviceSettings]
; MSI Support
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1

[igfx_RemoveDeviceSettings]

HKR,, VgaCompatible
HKR,, NativeResolution
HKR,, NativeBPP
HKR,, ConfigID
HKR,, PC_Release_Major
HKR,, PC_Release_Minor
HKR,, ApplyNativeMode
HKR,, DelayInPointerShapeChange

; Overlay specific settings
HKR,, Disable_OverlayDSQualityEnhancement

; Rotation specific settings
HKR,,   Display1_EnableRotation
HKR,,   Display1_RotationCaps
HKR,,   Display2_RotationCaps
HKR,,   Display1_IndependentRotation
HKR,,   Display1_EnableIndependentRotation
HKR,,   Display1_EnableIDDC_WA
HKR,,   RotationSPLCase
HKR,,   SmoothRotationSupport

; Event Manager specific settings
HKR,,    DisplayPriority
HKR,,     EDIDDefaultXX
HKR,,    EDIDDefaultYY
HKR,,    EDIDDefaultRR
HKR,,    EDIDDefaultBPP
HKR,,    LegacyDefaultXX
HKR,,    LegacyDefaultYY
HKR,,    LegacyDefaultRR
HKR,,    LegacyDefaultBPP

HKR,,    AStatePersistence
HKR,,    PerUserPersistence
HKR,,    UseBIOSDataforDock
HKR,,    HpDock
HKR,,    TMM_Active
HKR,,    RequestSig
HKR,,    RequestedXRes
HKR,,    RequestedYRes
HKR,,    RequestedBPP
HKR,,    RequestedRate

HKR,,    HotKeyPersistence
HKR,,    HotKeyPersistMDS
HKR,,    LidPersistence
HKR,,    DockPersistence
HKR,,    HotPlugPersistence
HKR,,    PowerPersistence
HKR,,    EdidPersistence
HKR,,    LFPAlwaysPrimary
HKR,,    OpenGLInstalled

;=====================================================================
; Device Common RegKey Enabling/Disabling
;=====================================================================
;=====================================================================
[Common_AddSwSettings]
;=====================================================================
;--OEMStaticMode_AddSwSettings-- 
; This shows number of Static modes to be used.
; TotalStaticModes = 0-->Disable the feature.
; Following keys have 8 bytes:
; 2B XRes + 2B YRes
; + 2B RRMask (Bit 0 - 60, 1 -70, 2 - 72, 3 - 75, 4 - 85,5 - 100,6 - 120,7-15 reserved)
; + 1B BppMask(Bit 0 - 8bpp,1 - 16bpp,2 - 32bpp, 3-7 reserved)
; + 1B reserved.
; all values in Hex; l->low byte, h->high byte
; Examples:
;                                  		      xl xh  yl yh  rl  rh  bp Rv
; HKR,, STATIC_MODE_1,%REG_BINARY%, 20,03,58,02,03,00,07,0F ; 8x6 60,70
; HKR,, STATIC_MODE_2,%REG_BINARY%, 20,03,58,02,20,00,04,0F ; 8x6 100 : 32bpp  

HKR,, TotalStaticModes, %REG_DWORD%, 0 
 
;--Underscan_AddSwSettings--
; 0 - default 7.5% under scan and OEM's can give under scan like 8,9 an 10  
HKR,, Display1_AddUnderscanPercentageHDMI,%REG_DWORD%, 0
  
;--HDMI_VSI_AddSwSettings--
HKR,, SPDIFVendorName,%REG_SZ%, "Intel" 	         ; max 8 characters
HKR,, SPDIFVendorDesc,%REG_SZ%, "9xxxx"	         ; max 16 characters
HKR,, HDMI_OptionalIFPriority,%REG_DWORD%, 0x21  ; default to priority 1 for SPD Infoframe and priority 2 for VS Infoframe
HKR,, HDMI_SupportCEA861D,%REG_DWORD%, 0        ;To enable support for 861D spec, 1-Support IT Content and RGB Quantization, 0- No 861D support. Default to 0. 

;-- NonEDIDMode_AddSwSettings--
; Following keys have 20 bytes (18 byte DTD + 2 Byte flags). The 2 bytes are as follows
; First byte
;   Bit 0 -> 8Bpp Support Bit; 0-Disabled, 1-Enabled
;   Bit 1 -> 16Bpp Support Bit; 0-Disabled, 1-Enabled
;   Bit 2 -> 32Bpp Support Bit; 0-Disabled, 1-Enabled
;   Bit 3 ->	 Bit 3 Reserved for any new BPP mask.
;   Bit 4 -> Bit for DFP Support ; 0-Disabled, 1-Enabled
;   Bit 5 -> Bit for CRT Support ; 0-Disabled, 1-Enabled
;   Bit 6-7 -> Bits 7-6 Reserved for Device Masks, must be 0
; Second Byte
;  Bit 0 -> DTD timing is added forcefully, even if timing is present in EDID.
;  Bit 1-7 -> Reserved Bits for any new masks
HKR,, DTD_1,%REG_BINARY%, 01,1D,80,18,71,1C,16,20,58,2C,1A,00,00,00,00,00,00,86,37,01        ; 1920x1080@60...Interlaced
HKR,, DTD_2, %REG_BINARY%, 01,1D,80,D0,72,1C,16,20,10,2C,1A,80,00,00,00,00,00,86,37, 01      ; 1920x1080@50...Interlaced
HKR,, DTD_3,%REG_BINARY%, 01,1D,00,BC,52,D0,1E,20,B8,28,25,40,00,00,00,00,00,04,37, 01       ; 1280x720@50....Non-interlaced
HKR,, DTD_4, %REG_BINARY%, 01,1D,00,72,51,D0,1E,20,6E,28,25,00,00,00,00,00,00,06,37,01        ; 1280x720@60....Non-interlaced
HKR,, DTD_5,%REG_BINARY%, 00, 00, 00 ,00, 00, 00,00, 00, 00,00, 00, 00,00, 00, 00,00, 00, 00,00, 00    ;Fifth DT

 HKR,, TotalDTDCount, %REG_DWORD%, 0   ; This shows number of DTDs to be used. ;  0-->Disable the feature.

;--CRTHotPlugDefaultVrefVoltage_AddSwSettings-- 
HKR,, Display1_EnableCRTHotPlugDefaultVrefVoltage,   %REG_DWORD%, 1  ; 1 - Enable(Default Value) and 0 - Disable(Customized Value)

;--AsyncFlips_AddSwSettings-- 
HKR,, Display1_DisableAsyncFlips,%REG_DWORD%, 0          ; 1 - Disable and 0 - Enable

;--DelayedDetectionForDP_AddSwSettings--
HKR,, DelayedDetectionForDP,%REG_DWORD%, 500         	  ; Delay in ms Range - 0 - 1000
 
;--DelayedDetectionForHDMI_AddSwSettings-- 
HKR,, DelayedDetectionForHDMI,%REG_DWORD%, 1000   	  ; Delay in ms Range - 0 - 1000
 
;--IncFixedSegWA_AddSwSettings-- 
HKR,, IncreaseFixedSegment,%REG_DWORD%, 0   	  ; 0 - disabled, 1- enabled 

;--EnableHDMIUnderScan_AddSwSettings-- 
HKR,, EnableHDMIUnderScan,%REG_DWORD%, 1              	  ; 1 - UnderScan and 0 - OverScan 
 
;--XVYCCFeature_AddSwSettings--
; When XVYCC feature is enabled, on corresponding display Hue and Saturation feature is disabled 
HKR,, XVYCCFeatureEnable,%REG_DWORD%, 0x01 ; 0x00- Disable, 0x01 - Enable... 
                       
;--WGFeature_AddSwSettings-- 
; When Wide Gamut feature is enabled, Hue and Saturation feature is disabled and xvYCC / Ycbcr is also disabled on HDMI
HKR,, WideGamutFeatureEnable,%REG_DWORD%, 0x00 	; 0x01- Enable for LFP, 0x02 - Enable for DP, 0x04 - Enable for HDMI... 

;<-NarrowGamut_AddSwSettings->
HKR,, NarrowGamutSplitGammaEnable,    %REG_DWORD%,    0x00 ;0x1 - Enable 0x0 - Disable 
;For Enabling Split Gamma in Narrow Gamut Feature , by default its disabled

;--DeepColorHDMI_AddSwSettings-- 
HKR,, DeepColorHDMIDisable,%REG_DWORD%, 0 	; 0- Enable Deep Color, 1 - Disable Deep Color

;--MediaRefreshRateMode_AddSwSettings-- 
HKR,, MediaRefreshRateMask, %REG_DWORD%, 0	 ; Mask to enable media refresh rates BIT0 - LFP BIT1-7 :Reserved

;--PdTogglingTimer_AddSwSettings-- 
HKR,, PdTogglingTimerValue,%REG_DWORD%, 0xBF   	  ; increasing the delay value.

;--eDPNoFLT_AddSwSettings-- 
; If this Registry is set to 1 then it will ignore the Fast Link Training and will always do Normal Link Training everytime
HKR,, NoFastLinkTrainingForeDP, %REG_DWORD%, 1

;--AUDIOWOVIDEOSupport_AddSwSettings--
HKR,, AudioWoVideoSupport,%REG_DWORD%, 0x01 	; 0x01- Enable, 0x00 - Disable
HKR,, AudioWoVideoStatus,%REG_DWORD%, 0x00	; 0x01- Enable, 0x00 - Disable 

;--AUDIOPERSISTENCE_AddSwSettings-- 
HKR,, DefaultAudioPolicyForClone,%REG_DWORD%, 0x01 	; 0x01- Cloned Audio Policy, 0x02 - Independent Audio Policy
HKR,, DefaultAudioPolicyForEDS,%REG_DWORD%, 0x02 	; 0x01- Cloned Audio Policy, 0x02 - Independent Audio Policy
HKR,, DriverUpgradeKey,%REG_DWORD%, 0x01 		; 0x01 - Driver Upgrade , Other values - Reboot
HKR,, AudioPointAggregationDelay,%REG_DWORD%, 0x0F 	; Delay in ms
HKR,, BasicAudioSupportForHDMI,%REG_DWORD%, 0x0 	; Default is 0. OEMs to make it one to explicitly check for this bit 
HKR,, AudioControllerEnableDelay,%REG_DWORD%, 0x1F4 ;Delay in ms

;--DisableCommonUserInterface_AddSwSettings-- 
HKR,, CUINotRequired, %REG_DWORD%, 0  		; 0x01 -  CUI will not be loaded 

;--Enable4KDisplay_AddSwSettings-- 
HKR,, Enable4KDisplay,%REG_DWORD%, 0x01		 ; 0x01- Enables 4K Display support, 0x00 - Disable 
HKR,, CollageModeFeature,%REG_DWORD%, 0x01	 ; bit 0 indicates the feature support, bit 1- indicates feature status in CUI(default is off)

;--DriverInstallState_AddSwSettings--
HKR,, Install_State, %REG_DWORD%, 0x1

;--igfx_TPV_AddSwSettings-- 
HKR,, TPVSolutionEnabled,       %REG_DWORD%,    1
HKR,, MAXViews,                 %REG_DWORD%,    2 
HKR,, MAXDevicesInView,         %REG_DWORD%,    2 
HKR,, MAXIntelDevicesActive,    %REG_DWORD%,    2 
HKR,, MAXOtherDevicesActive,    %REG_DWORD%,    3
HKR,, IsExtCloneSuppt,          %REG_DWORD%,    0

;--igfx_TPV_3Pipe_AddSwSettings--
HKR,, TPVSolutionEnabled,       %REG_DWORD%,    1
HKR,, MAXViews,                 %REG_DWORD%,    3 
HKR,, MAXDevicesInView,         %REG_DWORD%,    3 
HKR,, MAXIntelDevicesActive,    %REG_DWORD%,    3 
HKR,, MAXOtherDevicesActive,    %REG_DWORD%,    3
HKR,, IsExtCloneSuppt,          %REG_DWORD%,    0

;=====================================================================
[Common_DelSwSettings]
;=====================================================================
;--OEMStaticMode_DelSwSettings--
; HKR,, STATIC_MODE_1
; HKR,, STATIC_MODE_2
HKR,, TotalStaticModes

;--Underscan_DelSwSettings--
HKR,, Display1_AddUnderscanPercentageHDMI

;--HDMI_VSI_DelSwSettings--
HKR,, SPDIFVendorName
HKR,, SPDIFVendorDesc
HKR,, HDMI_OptionalIFPriority
HKR,, HDMI_SupportCEA861D

;--NonEDIDMode_DelSwSettings--
HKR,, TotalDTDCount
HKR,, DTD_1
HKR,, DTD_2
HKR,, DTD_3
HKR,, DTD_4
HKR,, DTD_5

;--CRTHotPlugDefaultVrefVoltage_DelSwSettings--
HKR,, Display1_EnableCRTHotPlugDefaultVrefVoltage

;--AsyncFlips_DelSwSettings--
HKR,, Display1_DisableAsyncFlips

;--DelayedDetectionForDP_DelSwSettings--
HKR,, DelayedDetectionForDP

;--DelayedDetectionForHDMI_DelSwSettings--
HKR,, DelayedDetectionForHDMI

;--IncFixedSegWA_DelSwSettings--
HKR,, IncreaseFixedSegment

;--EnableHDMIUnderScan_DelSwSettings--
HKR,, EnableHDMIUnderScan
 
;--XVYCCFeature_DelSwSettings--
HKR,, XVYCCFeatureEnable

;--WGFeature_DelSwSettings--
HKR,, WideGamutFeatureEnable

;<-NarrowGamut_DelSwSettings>
HKR,, NarrowGamutSplitGammaEnable

;--DeepColorHDMI_DelSwSettings--
HKR,, DeepColorHDMIDisable

;--MediaRefreshRateMode_DelSwSettings--
HKR,, MediaRefreshRateMask

;--PdTogglingTimer_DelSwSettings--
HKR,, PdTogglingTimerValue

;--eDPNoFLT_DelSwSettings--
HKR,, NoFastLinkTrainingForeDP

;--AUDIOWOVIDEOSupport_DelSwSettings--
HKR,, AudioWoVideoSupport
HKR,, AudioWoVideoStatus

;--AUDIOPERSISTENCE_DelSwSettings--
HKR,, DefaultAudioPolicyForClone
HKR,, DefaultAudioPolicyForEDS
HKR,, DriverUpgradeKey
HKR,, AudioPointAggregationDelay
HKR,, BasicAudioSupportForHDMI
HKR,, AudioControllerEnableDelay

;--DisableCommonUserInterface_DelSwSettings--
HKR,, CUINotRequired

;--Enable4KDisplay_DelSwSettings--
HKR,, Enable4KDisplay
HKR,, CollageModeFeature

;--DriverInstallState_DelSwSettings--
HKR,, Install_State

;--igfx_TPV_DelSwSettings--
HKR,, TPVSolutionEnabled
HKR,, MAXViews
HKR,, MAXDevicesInView
HKR,, MAXIntelDevicesActive
HKR,, MAXOtherDevicesActive
HKR,, IsExtCloneSuppt

;--igfx_TPV_3Pipe_DelSwSettings--
HKR,, TPVSolutionEnabled
HKR,, MAXViews
HKR,, MAXDevicesInView
HKR,, MAXIntelDevicesActive
HKR,, MAXOtherDevicesActive
HKR,, IsExtCloneSuppt

;--Enable3DContexts_IVBD0_DelSwSettings

;=====================================================================
[Common_Mobile_AddSwSettings]
;=====================================================================
;--General_AddSwSettings
; BitMask for Displays. If Set to 1, it indicates OEM Mode is preferred over EDID 
; Default Value is OEM is preferred over EDID
; Bit 0 - CRT:Bit 2 - DFP:Bit 1 and 3 reserved
HKR,, ModeEnumerationPreference,%REG_DWORD%, 0xFFFFFFFF    
                                                     
;--IntLVDSSwing_AddSwSettings--
; 0x00 - Medium - Data and Clk Swing set to 298 mV
; 0x01 - High - Data and Clk Swing set to 320 mV
; 0x02 - Low1 - Data and Clk Swing set to 144 mV
; 0x04 - Low2 - Data and Clk Swing set to 170 mV
; 0x08 - Low3 - Data and Clk Swing set to 196 mV
; 0x10 - Low4 - Data and Clk Swing set to 220 mV
; 0x20 - Low5 - Data and Clk Swing set to 247 mV
; 0x40 - Low6 - Data and Clk Swing set to 273 mV
HKR,, IntLVDSSwingSetting,%REG_DWORD%, 0x00 

;--PNM_AddSwSettings--
HKR,, PNMClkDeviation, %REG_DWORD%, 0   ; Clock deviation value which is multiplied by 10.
HKR,, PNMFlags, %REG_DWORD%, 0   	           ; Bit0: Downward Deviation, Bit1: Upward Deviation. Bit2-31: Reserved.

;--PwrCons_DPS_AddSwSettings--
HKR,, DPSCheckboxDefault,%REG_DWORD%, 0x1
HKR,, DPSBaseLoRRValue,%REG_DWORD%, 0x0
HKR,, Display1_DPSPanel_Type,%REG_DWORD%, 0xFF ;Normal/Static DRRS = 0, Seamless = 2, or Disable INF option = 0xFF
HKR,, DPSMotionArtifactMitigation,%REG_DWORD%, 0x1
HKR,, SupportForStaticDRRS,%REG_DWORD%, 0x0

;--Enable3DContexts_IVBM0_AddSwSettings--
; Game apps settings
HKR,, SupportAIL, %REG_DWORD%, 1
HKR,, @fifa.exe, %REG_DWORD%, 1
HKR,, @mnc.exe, %REG_DWORD%, 1
HKR,, @bf3.exe, %REG_DWORD%, 1
HKR,, @bf2.exe, %REG_DWORD%, 1
HKR,, @CivilizationV_DX11.exe, %REG_DWORD%, 1
HKR,, @NFS11.exe, %REG_DWORD%, 1
HKR,, @SSFIV.exe, %REG_DWORD%, 1
HKR,, @CoJGunslinger.exe, %REG_DWORD%, 1
HKR,, @F1_2012.exe, %REG_DWORD%, 1

;=====================================================================
[Common_Mobile_DelSwSettings]
;=====================================================================
;--General_DelSwSettings
HKR,, ModeEnumerationPreference
;--IntLVDSSwing_DelSwSettings
HKR,, IntLVDSSwingSetting
;--PNM_DelSwSettings
HKR,, PNMClkDeviation
HKR,, PNMFlags

;--PwrCons_DPS_DelSwSettings--
HKR,, DPSCheckboxDefault
HKR,, DPSControlMode
HKR,, DPSBaseLoRRValue
HKR,, Display1_DPSPanel_Type
HKR,, DPSMotionArtifactMitigation
HKR,, SupportForStaticDRRS

;--Enable3DContexts_IVBM0_DelSwSettings--
; Game apps settings
HKR,, SupportAIL
HKR,, @fifa.exe 
HKR,, @mnc.exe
HKR,, @bf3.exe
HKR,, @bf2.exe
HKR,, @CivilizationV_DX11.exe 
HKR,, @NFS11.exe 
HKR,, @SSFIV.exe 
HKR,, @CoJGunslinger.exe 
HKR,, @F1_2012.exe, %REG_DWORD%, 1

;=====================================================================
[Common_DT_AddSwSettings]
;=====================================================================
;--FakeEDID_AddSwSettings--
; EDID modified with private DTD for 357MHz max pixel rate, for eDP on Port D
HKR,, FakeEDID_14_0_af0d_1723,%REG_BINARY%,0,FF,FF,FF,FF,FF,FF,0,D,AF,23,17,0,0,0,0,2,15,1,4,95,26,15,78,2,D1,F5,93,5D,59,90,26,1D,50,54,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1D,36,80,A0,70,38,1E,40,2E,1E,24,0,7E,D7,10,0,0,18,0,0,0,5,0,74,8B,80,50,70,38,97,41,8,40,6,0,0,0,0,0,FE,0,43,4D,49,A,20,20,20,20,20,20,20,20,20,0,0,0,FE,0,4E,31,37,33,48,48,46,2D,45,32,31,20,20,0,39
HKR,, ReadEDIDFromRegistry, %REG_DWORD%, 1

;--Enable3DContexts_IVBD0_AddSwSettings--
; Workstation apps settings
HKR,, @acad.exe, %REG_DWORD%, 1
HKR,, @MstnBenchmark.exe, %REG_DWORD%, 1
; Game apps settings
HKR,, SupportAIL, %REG_DWORD%, 1
HKR,, @fifa.exe, %REG_DWORD%, 1
HKR,, @mnc.exe, %REG_DWORD%, 1
HKR,, @bf3.exe, %REG_DWORD%, 1
HKR,, @bf2.exe, %REG_DWORD%, 1
HKR,, @CivilizationV_DX11.exe, %REG_DWORD%, 1
HKR,, @NFS11.exe, %REG_DWORD%, 1
HKR,, @SSFIV.exe, %REG_DWORD%, 1
HKR,, @CoJGunslinger.exe, %REG_DWORD%, 1
HKR,, @F1_2012.exe, %REG_DWORD%, 1

;=====================================================================
[Common_DT_DelSwSettings]
;--FakeEDID_DelSwSettings--
HKR,, FakeEDID_14_0_af0d_1723
HKR,, ReadEDIDFromRegistry

;--Enable3DContexts_IVBD0_DelSwSettings--
; Workstation apps settings
HKR,, @acad.exe 
HKR,, @MstnBenchmark.exe
; Game apps settings
HKR,, SupportAIL
HKR,, @fifa.exe 
HKR,, @mnc.exe
HKR,, @bf3.exe
HKR,, @bf2.exe
HKR,, @CivilizationV_DX11.exe 
HKR,, @NFS11.exe 
HKR,, @SSFIV.exe 
HKR,, @CoJGunslinger.exe 
HKR,, @F1_2012.exe, %REG_DWORD%, 1

;=====================================================================
;  Device Specific Registry Keys
;=====================================================================
[Common_Device_Specific_DelSwSettings]
HKR,, FeatureTestControl
HKR,, MediaRefreshRateSupport
HKR,, AlternateScramblerSupport
HKR,, MediaRefreshRateSupport
HKR,, RsPipeGtRc6Settings
;--MediaRRSupport_DelSwSettings--
HKR,, MediaRefreshRateSupport
;--DisplayDPP_DelSwSettings--
HKLM,"SOFTWARE\Intel\IGFX\DPP"

;=====================================================================
[PwrCons_HSW_AddSwSettings]
HKR,, FeatureTestControl,%REG_DWORD%, 0xE200  ; Enable FBC, BLC, DPST, ALS, DRRS, RS, BLC DDI, Turbo, CxSR, PSR, DFPS

[MediaRRSupport_HSW_AddSwSettings]
HKR,, MediaRefreshRateSupport,%REG_DWORD%, 0x00     ;  bit7: reserved(0), bit6: reserved(0), bit5: 60 Hz , bit4: 50 Hz
                                                    ;  bit3: 48 Hz, bit2: 30 Hz, bit1: 25 Hz, bit0: 24 Hz

[AlternateScramblerSupport_HSW_AddSwSettings]
HKR,, AlternateScramblerSupport, %REG_DWORD%, 0x00

[DisplayDPP_HSW_AddSwSettings]
HKLM,"SOFTWARE\Intel\IGFX\DPP","SupportedDPP",%REG_DWORD%, 0x00  ;Uncomment the following values if SupportedDPP = 1
;HKLM,"SOFTWARE\Intel\IGFX\DPP","EnabledDPP",%REG_DWORD%, 0x00
;HKLM,"SOFTWARE\Intel\IGFX\DPP","EnabledManualMode",%REG_DWORD%, 0x00
;HKLM,"SOFTWARE\Intel\IGFX\DPP","AmbientKelvin",%REG_DWORD%, 0x1964		;Default value 6500
;HKLM,"SOFTWARE\Intel\IGFX\DPP","AmbientLux",%REG_DWORD%, 0x12C			;Default value 300
;HKLM,"SOFTWARE\Intel\IGFX\DPP","Brightness",%REG_DWORD%, 0x64			;Default value 100
;HKLM,"SOFTWARE\Intel\IGFX\DPP","SkinTone",%REG_DWORD%, 0x64			;Default value 100

[EnableDetachableEDPSupport_HSW_AddSwSettings]
HKR,, EnableDetachableEDPSupport, %REG_DWORD%, 0x00

[DisplayOptimization_HSW_AddSwSettings] 
; Bit0: Fastmodeset,  Bit1: T3 Optimization, Bit2: Power off optimization, Bit3: Link Training Optimization, Bit4: Sleep during T3 wait
HKR,, DisplayOptimizations, %REG_DWORD%, 0x1d

;=====================================================================
[PwrCons_BDW_AddSwSettings]
HKR,, FeatureTestControl,%REG_DWORD%, 0xF606	; Enable ALS, BLC, BLC DDI, CxSR, no FBC, DPST, DRRS, RS, PSR

[MediaRRSupport_BDW_AddSwSettings]
HKR,, MediaRefreshRateSupport,%REG_DWORD%, 0x00     ;  bit7: reserved(0), bit6: reserved(0), bit5: 60 Hz , bit4: 50 Hz
                                                    ;  bit3: 48 Hz, bit2: 30 Hz, bit1: 25 Hz, bit0: 24 Hz

[AlternateScramblerSupport_BDW_AddSwSettings]
HKR,, AlternateScramblerSupport, %REG_DWORD%, 0x00

[DisplayDPP_BDW_AddSwSettings]
HKLM,"SOFTWARE\Intel\IGFX\DPP","SupportedDPP",%REG_DWORD%, 0x00  ;Uncomment the following values if SupportedDPP = 1
;HKLM,"SOFTWARE\Intel\IGFX\DPP","EnabledDPP",%REG_DWORD%, 0x00
;HKLM,"SOFTWARE\Intel\IGFX\DPP","EnabledManualMode",%REG_DWORD%, 0x00
;HKLM,"SOFTWARE\Intel\IGFX\DPP","AmbientKelvin",%REG_DWORD%, 0x1964		;Default value 6500
;HKLM,"SOFTWARE\Intel\IGFX\DPP","AmbientLux",%REG_DWORD%, 0x12C			;Default value 300
;HKLM,"SOFTWARE\Intel\IGFX\DPP","Brightness",%REG_DWORD%, 0x64			;Default value 100
;HKLM,"SOFTWARE\Intel\IGFX\DPP","SkinTone",%REG_DWORD%, 0x64			;Default value 100

[EnableDetachableEDPSupport_BDW_AddSwSettings]
HKR,, EnableDetachableEDPSupport, %REG_DWORD%, 0x00

[DisplayOptimization_BDW_AddSwSettings] 
; Bit0: Fastmodeset,  Bit1: T3 Optimization, Bit2: Power off optimization, Bit3: Link Training Optimization, Bit4: Sleep during T3 wait
HKR,, DisplayOptimizations, %REG_DWORD%, 0x1d

;=====================================================================

[PwrCons_UserPolicy_DelSwSettings]
HKR,, ACPowerPolicyVersion
HKR,, DCPowerPolicyVersion
HKR,, PowerAcPolicy
HKR,, PowerDcPolicy
HKR,, ACUserPreferencePolicy
HKR,, DCUserPreferencePolicy
HKR,, ACSettingIndex
HKR,, DCSettingIndex
HKR,, TurboAcPolicy
HKR,, TurboDcPolicy
HKR,, PowerDpstAggressivenessLevel
HKR,, PowerGpsAggressivenessLevel

[AvoidPPSOutsideModeSet_AddSwSettings]
HKR,, AvoidPPSOutsideModeSet, %REG_DWORD%, 0x1 

[AvoidPPSOutsideModeSet_DelSwSettings]
HKR,, AvoidPPSOutsideModeSet

[DisableDisplayOptimization_AddSwSettings]
;for platforms that do not support optimization features this key can be used
HKR,, DisplayOptimizations, %REG_DWORD%, 0x0

[DisplayOptimization_DelSwSettings]
HKR,, DisplayOptimizations

[EnableDetachableEDPSupport_DelSwSettings]
HKR,, EnableDetachableEDPSupport
;
; Auto Notebook\Slate Convertible Specific Settings
;
[igfx_SLT_NB_AddSwSettings]
HKR,, ConvertibleSupport,       %REG_DWORD%,    0
HKR,, KeySltDockSupport,        %REG_DWORD%,    0

[igfx_SLT_NB_DelSwSettings]
HKR,, ConvertibleSupport
HKR,, KeySltDockSupport

;=====================================================================
;  End Add/Delete Registry entries
;=====================================================================
;
; Source file information
;
[SourceDisksNames]
1 = %DiskId%

[SourceDisksFiles]
igdkmd32.sys = 1
igd10iumd32.dll = 1
igdusc32.dll = 1
igdumdim32.dll = 1

[CUISDK.DelReg]
HKR,Igfxext
;  
; End CUI Registry Sections
;
[PowerPlanSettings]
;Intel Graphics Power Plan
Subgroup = {44F3BECA-A7C0-460e-9DF2-BB8B99E0CBA6}, "Intel(R) Graphics Settings", "Configure Intel(R) Graphics Settings"
Setting = {3619C3F2-AFB2-4afc-B0E9-E7FEF372DE36},"Intel(R) Graphics Power Plan", "Configure Intel(R) Graphics Power Plan"

Value = 0, "Maximum Battery Life", "Maximum Battery Life", %REG_DWORD%, 0
Value = 1, "Balanced", "Balanced", %REG_DWORD%, 1
Value = 2, "Maximum Performance", "Maximum Performance", %REG_DWORD%, 2

Default = %GUID_MAX_POWER_SAVINGS%, %AC%, 0
Default = %GUID_MAX_POWER_SAVINGS%, %DC%, 0
Default = %GUID_TYPICAL_POWER_SAVINGS%, %AC%, 1
Default = %GUID_TYPICAL_POWER_SAVINGS%, %DC%, 1 
Default = %GUID_MIN_POWER_SAVINGS%, %AC%, 2
Default = %GUID_MIN_POWER_SAVINGS%, %DC%, 2

[Strings]
;DPPE
GUID_MAX_POWER_SAVINGS = "{a1841308-3541-4fab-bc81-f71556f20b4a}"
GUID_TYPICAL_POWER_SAVINGS = "{381b4222-f694-41f0-9685-ff5bb260df2e}"
GUID_MIN_POWER_SAVINGS = "{8c5e7fda-e8bf-4a96-9a85-a6e23a8c635c}"
AC = 0
DC = 1

;
; Customizable Strings
;
CUIDeviceIndependentKey="Software\Intel\Display\igfxcui"
DisplayKey="Software\Intel\Display"
CUIDriverOldShareKey="Software\Intel\CUI"
;
; Non-Localizable Strings
;
REG_SZ         = 0x00000000
REG_SZNAT      = 0x00020007
REG_MULTI_SZ   = 0x00010000
REG_DWORD      = 0x00010001
REG_BINARY     = 0x00000001
SERVICEROOT    = "System\CurrentControlSet\Services"
;
; Localizable Strings
;
DiskId      	= "Intel(R) Graphics Media Accelerator Driver for Windows"
Intel        	= "Intel Corporation"
; HSW A0/A1
iHSWGTLD    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTL"
iHSWGTLM    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTL"
iHSWGTMD   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTM"
iHSWGTMM   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTM"
iHSWGTHD   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTH"
iHSWGTHM   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics - GTH"
; HSW Classic
iHSWGT1D   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics"
iHSWGT1M    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics"
iHSWGT15D    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 4400"
iHSWGT2D    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
iHSWGT2M    	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
; HSW ULT
iHSWGT1UT   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics"
iHSWGT2UT   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics Family"
iHSWGT3UT   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 5000"
iHSWGT3UT25W   	= "(PE) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5100"
iHSWGT2UX   	= "(PE) Intel(R) 4th Generation Haswell HD Graphics Family"
iHSWGT1ULX	= "(PE) Intel(R) 4th Generation Haswell HD Graphics"
; HSW CRW
iHSWGT2CW  	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
iHSWGT2CWDT  	= "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
iHSWGT3CW  	= "(PE) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5200 with High Speed Memory"
iHSWGT3CWDT  	= "(PE) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5200 with High Speed Memory"
; HSW SRVR
iHSWSVGT1  	= "(PE) Intel(R) 4th Generation Haswell HD Graphics"
iHSWSVGT2  	= "(PE) Intel(R) 4th Generation Haswell HD Graphics P4600/P4700"
; BDW Simulation
iBDWGD0     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS"
iBDWGT0     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS GT0"
iBDWGT1     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS GT1"
iBDWGT2     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS GT2"
iBDWGT3     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS GT3"
iBDWGT4     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics HAS GT4"
; BDW HW
iBDWMULTGT1 = "(PE) Intel(R) 5th Generation Broadwell HD Graphics M ULT GT1"
iBDWULXGT1  = "(PE) Intel(R) 5th Generation Broadwell HD Graphics ULX GT1"
iBDWMULTGT2 = "(PE) Intel(R) 5th Generation Broadwell HD Graphics M ULT GT2"
iBDWULXGT2  = "(PE) Intel(R) 5th Generation Broadwell HD Graphics ULX GT2"
iBWDHALOGT1 = "(PE) Intel(R) 5th Generation Broadwell HD Graphics Halo GT1"
iBWDHALOGT2 = "(PE) Intel(R) 5th Generation Broadwell HD Graphics Halo GT2"
iBWDHALOGT3 = "(PE) Intel(R) 5th Generation Broadwell HD Graphics Halo GT3"
;
; Do not modify or copy the following line
; set SIGNING_KEY_VERSION=2
;                                   