
       Оптимизированный драйвер INTEL Graphics 20.19.15.4444 для использования в PE_7/8/8.1/10x32.

    Драйвер пригоден для установщика DevInst, SDI или стандартного обновления устройств.

    Для стандартного обновления устройств распакуйте драйвер до уровня каталогов с файлами.


--------------------------------------------------------------------------------------------------

      Драйвер INTEL Graphics 20.19.15.4444 Windows 7/8/8.1/10 (32 bit), каталог IG2019154444_NT6x32.     

    DriverVer=04/22/2016, 20.19.15.4444. Отключены OpenCL, OpenGL, ControlPanel, WiDi Miracast.

    Product Support:

     6th Generation Intel® Core™ processor family (codename Skylake)
     5th Generation Intel® Core™ processor family (codename Broadwell)
     CherryView Intel® processor family (Braswell)

     Intel® Xeon® Processor E3-1500 v5 Product Family (codename Skylake)
     Intel® Xeon® Processor E3-1200 v5 Product Family (codename Skylake)

    Для Windows 8.1 используется секция igfx_SoftwareDX11Settings вместо igfx_SoftwareDX12Settings

--------------------------------------------------------------------------------------------------

     ; BDW HW
     iBDWULTGT1	     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics" 
     iBDWULTGT2      = "(PE) Intel(R) 5th Generation Broadwell HD Graphics 5500" 
     iBDWULTGT3      = "(PE) Intel(R) 5th Generation Broadwell HD Graphics 6000" 
     iBDWULXGT1      = "(PE) Intel(R) 5th Generation Broadwell HD Graphics" 
     iBDWULXGT2      = "(PE) Intel(R) 5th Generation Broadwell HD Graphics 5300" 
     iBDWHALOGT2     = "(PE) Intel(R) 5th Generation Broadwell HD Graphics 5600" 
     iBDWHALOGT3     = "(PE) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics 6200" 
     iBDWGT3SRVR     = "(PE) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics P6300" 
     iBDWGT2SRVR     = "(PE) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics P6300" 
     iBDWULTGT328W   = "(PE) Intel(R) 5th Generation Broadwell Iris(TM) Graphics 6100" 
     
     ; CHV HW  
     iCHVGM0         = "(PE) Intel(R) CherryView (Braswell) HD Graphics" 
     iCHVGM1         = "(PE) Intel(R) CherryView (Braswell) HD Graphics" 
     
     ; SKL HW
     iSKLDTGT1       = "(PE) Intel(R) 6th Gen Skylake HD Graphics 510" 
     iSKLDTGT15      = "(PE) Intel(R) 6th Gen Skylake HD Graphics 530" 
     iSKLDTGT2       = "(PE) Intel(R) 6th Gen Skylake HD Graphics 530" 
     iSKLDTGT4       = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Pro Graphics P570\580" 
     iSKLULTGT1      = "(PE) Intel(R) 6th Gen Skylake HD Graphics 510" 
     iSKLULTGT15     = "(PE) Intel(R) 6th Gen Skylake HD Graphics 510"  
     iSKLULTGT2      = "(PE) Intel(R) 6th Gen Skylake HD Graphics 520" 
     iSKLULTGT2f     = "(PE) Intel(R) 6th Gen Skylake HD Graphics 520" 
     iSKLULTGT3      = "(PE) Intel(R) 6th Gen Skylake HD Graphics 535" 
     iSKLULTGT328W   = "(PE) Intel(R) 6th Gen Skylake HD Graphics 535" 
     iSKLULTGT3e     = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Graphics 540" 
     iSKLSRVGT1      = "(PE) Intel(R) 6th Gen Skylake HD Graphics SRV GT1" 
     iSKLSRVGT2      = "(PE) Intel(R) 6th Gen Skylake HD Graphics SRV GT2" 
     iSKLSRVGT3      = "(PE) Intel(R) 6th Gen Skylake HD Graphics SRV GT3" 
     iSKLSRVGT3e     = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Graphics P555" 
     iSKLSRVGT4      = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Pro Graphics P580" 
     iSKLULXGT1      = "(PE) Intel(R) 6th Gen Skylake HD Graphics ULX GT1" 
     iSKLULXGT15     = "(PE) Intel(R) 6th Gen Skylake HD Graphics ULX GT1.5" 
     iSKLULXGT2      = "(PE) Intel(R) 6th Gen Skylake HD Graphics 515" 
     iSKLHaloGT1     = "(PE) Intel(R) 6th Gen Skylake HD Graphics 510" 
     iSKLHaloGT2     = "(PE) Intel(R) 6th Gen Skylake HD Graphics 530" 
     iSKLHaloGT3fe   = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Graphics 555" 
     iSKLHaloGT4     = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Pro Graphics 580" 
     iSKLWSGT2       = "(PE) Intel(R) 6th Gen Skylake HD Graphics P530" 
     iSKLWSGT4       = "(PE) Intel(R) 6th Gen Skylake Iris(TM) Pro Graphics P580" 

--------------------------------------------------------------------------------------------------

 При использовании драйверов Intel Graphics необходимо учитывать поддержку в ОС от производителя.

По указанной ссылке, можно узнать поддерживается ли видеоадаптер в определенной операционной системе.

http://www.intel.ru/content/www/ru/ru/support/graphics-drivers/000005526.html


В РЕ-модификации драйверов Intel Graphics есть особенности. В зависимости от алгоритма определения

активного монитора оборудованием системной платы, может наблюдаться вывод изображения на "неосновной"

экран. Так, например, на некоторых системных платах Gigabyte, после инициализации драйвера, изображение 

пропадает с DB-15 разъема(обычный 15-пиновый) и появляется на цифровом HDMI к которому ничего не

подключено. На некоторых ноутбуках\моноблоках после установки драйвера изображение "переходит" на

разъем для внешнего монитора, что сопровождается явлением "черного экрана" на основной панели.   

==================================================================================================
 14-Jun-2017 nat27 http://forum.ru-board.com/topic.cgi?forum=62&topic=24098&start=71&limit=1&m=1#1
==================================================================================================
  